For 1990-2009 cars

#### Special Tools

EN-48252 Installer Camshaft Oil Seal

For equivalent regional tools, refer to Special Tools.

1. Install a NEW camshaft oil seal (1) to the cylinder head (2).
2. Use the EN-48252 installer (1) to install the camshaft oil seal.
3. Install the camshaft oil seal (1).

Note: While installing the camshaft oil seal (1) to the cylinder head (2) it is importantly that the camshaft oil seal concisely at the cylinder head fits.