For 1990-2009 cars

The driver and passenger power seat systems each consist of the following components:

• | Seat Adjuster Switch

• | Seat Horizontal Motor

• | Seat Front Vertical Motor

• | Seat Rear Vertical Motor

• | Seat Recline Motor

• | CB2 circuit breaker 25 A

### Seat Adjuster Switch

The seat adjuster switches provide both power and ground to the selected seat motors. Battery positive voltage is supplied at all times to the driver and passenger seat adjuster switches from the CB2 circuit breaker located in the I/P fuse block. The driver and passenger seat adjuster switches receives ground through the switch ground circuit and G307.

### Motors

All of the seat motors operate independently of each other. Each motor contains an electronic circuit breaker (PTC) that opens in the event of a circuit overload and will reset only after voltage has been removed from the circuit. There are four seat position motors. These are the horizontal motor, front vertical motor, rear vertical motor, and the seat back recline motor. The horizontal motor moves the entire seat forward and rearward. The seat vertical motors may operate independently to tilt the front or rear of the seat cushion up or down. Both motors can also run simultaneously to move the entire seat up or down. The recline motor moves the angle of the seat back forward or rearward.

### Horizontal

When the seat switch is operated to move the entire seat forward, battery positive voltage is applied through the switch contacts and the horizontal motor forward control circuit to the motor. The motor is grounded through the horizontal motor rearward switch contacts and the horizontal motor rearward control circuit to the motor. The motor runs in order to drive the entire seat forward until the switch is released. Moving the entire seat rearward works similarly to moving the entire seat forward, except that battery positive voltage and ground are applied on opposite circuits causing the motor to run in the opposite direction.

### Rear Vertical

When the seat switch is operated to tilt the rear of the seat cushion up, battery positive voltage is applied through the switch contacts and the rear vertical motor up control circuit to the rear vertical motor. The motor is grounded through the down switch contacts and the rear vertical motor down control circuit to the motor. The motor runs in order to drive the rear of the seat cushion up until the switch is released. Tilting the rear of the seat cushion down works similarly to tilting the rear of the seat cushion up, except that battery positive voltage and ground are applied on opposite circuits causing the motor to run in the opposite direction.

### Front Vertical

When the seat switch is operated to tilt the front of the seat cushion up, battery positive voltage is applied through the switch contacts and the front vertical motor up control circuit to the motor. The motor is grounded through the down switch contacts and the front vertical motor down control circuit to the motor. The motor runs in order to drive the front of the seat cushion up until the switch is released. Tilting the front of the seat cushion down works similarly to tilting the front of the seat cushion up, except that battery positive voltage and ground are applied on opposite circuits causing the motor to run in the opposite direction.

### Entire Seat Up or Down

When the seat switch is operated in order to move the entire seat to the up position, battery positive voltage is simultaneously applied through the front and rear vertical motor up switch contacts and the front and rear vertical motor up control circuits to both vertical motors. The motors are grounded through the down switch contacts and the front and rear vertical motor down control circuits to both vertical motors. Both motors run simultaneously in order to drive the entire seat up until the switch is released. Moving the entire seat down works similarly to moving the entire seat up, except that battery positive voltage and ground are applied on the opposite circuits causing the motors to run in the opposite direction.

### Recline

When the seat recline switch is operated to move the seat back forward, battery positive voltage is applied through the switch contacts and the recline motor forward control circuit to the motor. The motor is grounded through the rearward switch contacts and the recline motor rearward control circuit to the motor. The motor runs in order to move the seat back forward until the switch is released. Moving the seat back rearward works similarly to moving the seat back forward, except that battery positive voltage and ground are applied on the opposite circuits causing the motor to run in the opposite direction.