For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect and connect battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Battery Positive Cable to Fuse Box Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Battery Positive Cable to Battery Nut Tighten 9 N·m(80 lb in)
3 | Battery Positive from Battery to Fuse Box Cable