For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Side Door Check Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m(19 lb ft)
2 | Front Side Door Weatherstrip - Door Side

#### Procedure

1. Unclip weatherstrip from front side door.
2. When removing protective liners from adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.