For 1990-2009 cars

NEED GRAPHIC

Callout | Component Name
--- | ---
1 | Bolt Access Plug

#### Procedure

Use a plastic flat-bladed tool to remove.

2 | Front Side Door Outside Handle Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten XX N·m(XX lb ft)
3 | Front Door Outside Handle Cap
4 | Front Door Outside Handle Cap Gasket
5 | Front Door Outside Handle

#### Procedure

Pull the outside handle rearward to release it from the inside handle housing.

6 | Front Door Outside Handle Gasket

#### Procedure

Inspect the lock, lock cylinder and handle adjustments. Refer to Front Side Door Outside Handle Rod Adjustment.