For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the headlining trim panel. Refer to Headlining Trim Panel Replacement.
2. Remove the sunroof window. Refer to Sunroof Window Replacement.
3. Remove the sunroof air deflector cover. Refer to Sunroof Air Deflector Cover Replacement.
4. Remove the sunroof sunshade. Refer to Sunroof Sunshade Replacement.
5. Remove the sunroof window motor. Refer to Sunroof Window Motor Replacement.

1 | Sunroof Module Bolt (Qty: 12) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Sunroof Frame

#### Procedure

With the aid of an assistant, lower the sunroof frame and remove the sunroof frame out through the passenger side door.