For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front bumper fascia. Refer to LINK.
3. Disconnect fog lamp bulb socket electrical connector.

1 | Front Fog Lamp Screws (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten xx N·m (xx lb ft)
2 | Front Fog Lamp Assembly

#### Procedure

1. Remove the lamp assembly from the fog lamp bracket.
2. Aim the fog lamp after installation. Refer to Fog Lamp Aiming.