For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.

1 | Front Side Door to Roof 6.0 mm ± 1.0 mm (0.24 in ± 0.04 in) Caution: Refer to Fastener Caution in the Preface section. Tip

1. Loosen the Front Side Door Hinge Bolt (Qty: 4) to adjust the front side door.
2. Adjust the front side door in order to obtain an even gap between the front side door and the roof, the rear door, the rocker panel and the front fender and so that the front side door is flush with the roof, the rear door, the rocker panel and the front fender.

Tighten
25 N·m(19 lb ft)

2 | Front Side Door to Rear Door 3.5 mm ± 0.75 mm (0.14 in ± 0.03 in)
3 | Front Side Door to Rocker Panel 4.5 mm ± 1.0 mm (0.18 in ± 0.04 in)
4 | Front Side Door to Front Fender 3.5 mm ± 0.75 mm (0.14 in ± 0.03 in)