For 1990-2009 cars

1. Remove the 8 connecting rod bearing cap bolts (3).

Note: Mark and confirm the connecting rod bearing cap (1) position to ensure they are installed in the same position for assembly. Apply identification mark if not present.

2. Remove the 4 connecting rod bearing caps (2).

Note: Take extreme care to prevent damage to the cylinder bore surface, piston ring and piston surface.

3. Remove the 4 pistons with 4 connecting rods (1) push to the top of the engine block.

Note:

• | Mark the position of theconnecting rod bearings (4) for assembly.

• | Take extreme care to prevent any scratches or damages to the connecting rod bearings.

4. Remove the 8 connecting rod bearings (4).