For 1990-2009 cars

1. Remove the radiator. Refer to Radiator Replacement.
2. Remove the charge air cooler. Refer to Charge Air Cooler Replacement.
3. Drill hole in the charge air cooler bracket and radiator bracket (2) using a 7 mm (0.28 in) drill.
4. Install the j-clip (3) to the radiator.
5. Install the radiator. Refer to Radiator Replacement.
6. Install the charge air cooler to the radiator. Refer to Engine Coolant Fan Replacement.
7. Install the repair bolt (1) with locking compound.