For 1990-2009 cars

#### Special Tool

EN 845 Suction Device

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Remove the camshaft. Refer to Camshaft Replacement.

Note: Mark the assignments.

2. Remove the 16 valve lifter (1) use the EN 845 suction device .

### Installation Procedure

Note: Observe the correct assignment.

Note: Coat the sliding surfaces with NEW engine oil.

1. Install the 16 valve lifter (1) use the EN 845 suction device .
2. Install the camshaft. Refer to Camshaft Replacement.