For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment sill trim plate. Refer to Rear Compartment Sill Trim Plate Replacement.

1 | Rear Compartment Lid Latch Striker Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use a grease pencil to outline the striker before removing the bolts.

Tighten
XX N·m(XX lb ft)

2 | Rear Compartment Lid Latch Striker

#### Procedure

Adjust the rear compartment lid latch striker after replacing, if needed.