For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation.

1 | Stabilizer Shaft Link Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 65 N·m (48 lb ft)
2 | Stabilizer Shaft Link