For 1990-2009 cars

Figure 1: |

#### X102 Body Front Harness & Engine Cooling Harness

#### Connector Part Information

- Harness: Engine Cooling
- OEM: -
- Service: -
- Description: 4-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X102 Body Front Harness & Engine Cooling Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 4 Yellow | 5358 | Cooling Fan Motor Control (3) (LLW)
4 Yellow | 5358 | Cooling Fan Motor Control (3) (LXT)
4 Yellow | 5358 | Cooling Fan Motor Control (3) (D)
4 Yellow | 5358 | Cooling Fan Motor Control (3) (FI)
4 Yellow | 5358 | Cooling Fan Motor Control (3) (LXV LDE 2H0)
2 | 2.5 Gray | 532 | Cooling Fan Motor Control (2) (LLW)
2.5 Gray | 532 | Cooling Fan Motor Control (2) (LXT)
2.5 Gray | 532 | Cooling Fan Motor Control (2) (D)
2.5 Gray | 532 | Cooling Fan Motor Control (2) (FI)
2.5 Gray | 532 | Cooling Fan Motor Control (2) (LXV LDE 2H0)
3 | 4 White-Black | 2366 | Cooling Fan Control Relay Speed Signal (LLW)
2.5 White-Blue | 409 | Cooling Fan Motor Control (1)
2.5 White-Blue | 409 | Cooling Fan Motor Control (1) (LXV LDE 2H0)
2.5 White-Blue | 409 | Cooling Fan Motor Control (1) (LXT)
4 | 0.75 Brown-Green | 59 | A/C Compressor Clutch Control
0.5 Brown-Green | 59 | A/C Compressor Clutch Control (LXT)

Figure 2:

#### X104 Body Front Harness & Engine Cooling Harness

#### Connector Part Information

- Harness: Engine Cooling
- OEM: -
- Service: -
- Description: 5-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X104 Body Front Harness & Engine Cooling Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 Green | 380 | A/C Refrigerant Pressure Sensor Signal (LDE/LXV/2H0)
0.5 Green | 380 | A/C Refrigerant Pressure Sensor Signal (LLW)
0.5 Green | 380 | A/C Refrigerant Pressure Sensor Signal (LXT)
2 | 0.5 Brown-Red | 2700 | A/C Pressure Sensor 5 Volt Reference (LDE/LXV/2H0)
0.5 Brown-Red | 2700 | A/C Pressure Sensor 5 Volt Reference (LLW)
0.5 Brown-Red | 2700 | A/C Pressure Sensor 5 Volt Reference (LXT)
3 | 0.5 Black-Brown | 5514 | A/C Refrigerant Pressure Sensor Low Reference (LDE/LXV/2H0)
0.5 Black-Brown | 5514 | A/C Refrigerant Pressure Sensor Low Reference (LLW)
0.5 Black-Brown | 5514 | A/C Refrigerant Pressure Sensor Low Reference (LXT)
4 | 0.5 Green-Violet | 2032 | Coolant Temperature Sensor Signal (LDE/LXV/2H0)
5 | 0.5 Black-Blue | 6813 | Coolant Temperature Sensor #2 Low Reference (LDE/LXV/2H0)

Figure 3:

#### X114 Body Harness & Electrical Power Steering Harness

#### Connector Part Information

- Harness: Power Steering
- OEM: -
- Service: -
- Description: 12-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X114 Body Harness & Electrical Power Steering Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 Blue | 2500 | High Speed GMLAN Serial Data (+) (1)
B | 0.5 White | 2501 | High Speed GMLAN Serial Data (-) (1)
C | 0.5 Blue | 2500 | High Speed GMLAN Serial Data (+) (1)
D | 0.5 White | 2501 | High Speed GMLAN Serial Data (-) (1)
K | 0.5 White-Blue | 5986 | Serial Data Communication Enable

Figure 4:

#### X114 Body Harness & Electrical Power Steering Harness

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 12-Way Male (Black/Violet)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X114 Body Harness & Electrical Power Steering Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 Blue | 2500 | High Speed GMLAN Serial Data (+) (1) (NJ1)
B | 0.5 White | 2501 | High Speed GMLAN Serial Data (-) (1) (NJ1)
C | 0.5 Blue | 2500 | High Speed GMLAN Serial Data (+) (1) (NJ1)
D | 0.5 White | 2501 | High Speed GMLAN Serial Data (-) (1) (NJ1)
K | 0.5 White-Blue | 5986 | Serial Data Communication Enable (NJ1)

Figure 5:

#### X115 Body Harness & Electrical Power Steering Harness (NJ1)

#### Connector Part Information

- Harness: Power Steering
- OEM: -
- Service: -
- Description: 2-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X115 Body Harness & Electrical Power Steering Harness (NJ1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 6:

#### X115 Body Harness & Electrical Power Steering Harness (NJ1)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 2-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X115 Body Harness & Electrical Power Steering Harness (NV7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 6 Black | 50 | Ground
0.5 Brown-Green | 1295 | Variable Effort Steering Solenoid Control
B | 0.5 Black-Yellow | 6641 | Variable Effort Steering Solenoid Low Reference

Figure 7:

#### X115 Body Harness & Electrical Power Steering Harness (NV7)

#### Connector Part Information

- Harness: Power Steering
- OEM: -
- Service: -
- Description: 2-Way Female (-)

#### Terminal Part Information

- Pins:
- Terminated Lead: Service by Connector Assembly
- Release Tool: 15315247
- Diagnostic Test Probe: J-35616-2A (GY)

#### X115 Body Harness & Electrical Power Steering Harness (NV7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 8:

#### X115 Body Harness & Electrical Power Steering Harness (NV7)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 2-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X115 Body Harness & Electrical Power Steering Harness (NV7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 9:

#### X200 Body Harness & Instrument Panel Harness

#### Connector Part Information

- Harness: Instrument panel Instrument panel
- OEM: -
- Service: -
- Description: 102-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X200 Body Harness & Instrument Panel Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.75 Blue-Yellow | 1960 | Front Center Speaker (-) (UQG)
2 | 0.75 Yellow-White | 1860 | Front Center Speaker (+) (UQG)
8 | 0.5 Brown-Black | 3552 | Passive Start Interior Antenna 1 Signal Hi
9 | 0.5 Blue | 3554 | Passive Start Interior Antenna 2 Signal Hi
10 | 0.5 Gray-Black | 3555 | Passive Start Interior Antenna 2 Signal Lo
11 | 0.5 White | 3553 | Passive Start Interior Antenna 1 Signal Lo
12 | 0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (LHD UQG)
0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (RHD UQG)
13 | 0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (LHD UQG)
0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (RHD UQG)
14 | 0.75 Green-Black | 116 | Left Rear Speaker Signal (-) (LHD UQG)
0.75 Green-Black | 116 | Left Rear Speaker Signal (-) (RHD UQG)
15 | 0.75 Blue-Black | 115 | Right Rear Speaker Signal (-) (LHD UQG)
0.75 Blue-Black | 115 | Right Rear Speaker Signal (-) (RHD UQG)
16 | 0.5 Violet-Black | 7553 | Park Lock Solenoid Control
17 | 0.5 Violet-Black | 3 | Ignition Voltage (ATH)
19 | 0.5 Blue-Yellow | 6105 | High Speed GMLAN Serial Data (+) (2)
20 | 0.5 White | 6106 | High Speed GMLAN Serial Data (-) (2)
21 | 0.5 Red-White | 40 | Battery Positive Voltage
22 | 0.5 Yellow | 40 | Battery Positive Voltage
23 | 0.75 Blue | 201 | Left Front Speaker (+) (1) (LHD UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (RHD UQG)
24 | 0.75 Yellow | 200 | Right Front Speaker (+) (1) (LHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (RHD UQG)
25 | 0.75 Green | 199 | Left Rear Speaker (+) (LHD UQG)
0.75 Green | 199 | Left Rear Speaker (+) (RHD UQG)
26 | 0.75 White | 46 | Right Rear Speaker (+) (LHD UQG)
0.75 White | 46 | Right Rear Speaker (+) (RHD UQG)
27 | 1 Blue-Violet | 807 | OFF /Accessory Voltage
1 Blue-Violet | 807 | OFF /Accessory Voltage (-ATH)
28 | 0.5 Violet-Yellow | 4 | Ignition Voltage (ATH)
29 | 0.5 Black-Gray | 6110 | Clutch Apply Sensor Low Reference
30 | 0.5 Yellow | 6111 | Clutch Apply Sensor Signal
31 | 0.5 Gray-Red | 6109 | Clutch Apply Sensor Voltage Reference
32 | 0.5 Yellow | 7546 | Logistics Relay Control
0.5 Yellow | 7546 | Logistics Relay Control (UAG/UFD)
0.5 Yellow | 7546 | Logistics Relay Control (UDK)
33 | 0.35 Gray-Green | 7565 | Windscreen Temp Sensor Signal (CJ2)
34 | 0.5 Red-Brown | 40 | Battery Positive Voltage (ATH)
0.5 Red-Violet | 40 | Battery Positive Voltage (ATH)
35 | 0.5 Dark Green | 5103 | Technology Identification
0.5 Green-Black | 5103 | Technology Identification
0.5 Green-Black | 5103 | Technology Identification (UAG/UFD)
0.5 Green-Black | 5103 | Technology Identification (UDK)
36 | 0.5 Yellow-Green | 3274 | Remote Function Actuator Transmit Signal
37 | 0.5 Blue-White | 3275 | Remote Function Actuator Receive Signal
38 | 0.5 Gray-White | 3272 | Remote Function Actuator Supply Voltage
39 | 0.5 Gray | 3273 | Remote Function Actuator Return
40 | 0.75 Green-Violet | 1601 | Steering Column Lock Signal
41 | 0.5 Blue-Gray | 636 | Outside Ambient Air Temperature Sensor Signal
42 | 0.5 Green-Black | 3358 | Left TV Audio Return (ATH)
0.5 Green-Black | 3558 | Passive Start Switch Signal 2 (ATH)
43 | 0.5 Black-Gray | 3359 | Right TV Audio Return (ATH)
0.5 Black-Gray | 3559 | Passive Start Switch 2 Low Reference (ATH)
44 | 0.35 Yellow-Blue | 3197 | Humidity Temperature Sensor Signal (CJ2)
45 | 0.5 Yellow-White | 1161 | Accelerator Pedal Position Signal (1) (LDE/LXV/2H0)
0.5 Yellow-White | 1161 | Accelerator Pedal Position Signal (1) (LLW)
0.5 Yellow-White | 1161 | Accelerator Pedal Position Signal (1) (LXT -SAE)
46 | 0.5 Black-Blue | 1271 | Accelerator Pedal Position Low Reference (1) (LDE/LXV/2H0)
0.5 Black-Blue | 1271 | Accelerator Pedal Position Low Reference (1) (LLW)
0.5 Black-Blue | 1271 | Accelerator Pedal Position Low Reference (1) (LXT -SAE)
47 | 0.5 Black-Violet | 1272 | Accelerator Pedal Position Low Reference (2) (LDE/LXV/2H0)
0.5 Black-Violet | 1272 | Accelerator Pedal Position Low Reference (2) (LLW)
0.5 Black-Violet | 1272 | Accelerator Pedal Position Low Reference (2) (LXT -SAE)
48 | 0.5 Green-White | 1162 | Accelerator Pedal Position Signal (2) (LDE/LXV/2H0)
0.5 Green-White | 1162 | Accelerator Pedal Position Signal (2) (LLW)
0.5 Green-White | 1162 | Accelerator Pedal Position Signal (2) (LXT -SAE)
49 | 0.5 Black-Blue | 61 | Outside Ambient Temperature Sensor Low Reference
50 | 0.35 Violet-White | 5203 | Air Quality Sensor Signal
51 | 0.5 Green-Gray | 6135 | Linear Interconnect Network Bus 4
52 | 0.5 Violet-Green | 39 | Ignition Voltage
53 | 0.5 Violet-Green | 39 | Ignition Voltage
0.5 Violet-Green | 3039 | Run/Crank Ignition 1 Voltage
54 | 0.5 Red-Green | 40 | Battery Positive Voltage
55 | 0.5 Red-Blue | 40 | Battery Positive Voltage
0.5 Red-Blue | 840 | Battery Positive Voltage
57 | 0.5 Brown-Yellow | 39 | Ignition Voltage
0.5 Brown-Yellow | 239 | Ignition Voltage
58 | 0.75 Gray-Yellow | 6188 | Lift Glass/Trunk Motor Release Control
59 | 1 White-Brown | 6815 | Inadvertent Power Control
60 | 0.5 Brown-Yellow | 189 | Headlamp Leveling Motor Control
61 | 0.5 Brown-Violet | 193 | Rear Defog Relay Control
62 | 0.35 Black-Blue | 7566 | Humidity/Windscreen Temp Sensor Low Reference (CJ2)
0.35 Dark Green | 50 | Ground
63 | 0.35 Gray-Blue | 7564 | Humidity Sensor Signal (CJ2)
64 | 0.35 Yellow-Red | 597 | 5 Volt Reference (CJ2)
65 | 0.5 Brown-Red | 1274 | Accelerator Pedal Position 5 Volt Reference (2) (LDE/LXV/2H0)
0.5 Brown-Red | 1274 | Accelerator Pedal Position 5 Volt Reference (2) (LLW)
0.5 Brown-Red | 1274 | Accelerator Pedal Position 5 Volt Reference (2) (LXT -SAE)
66 | 0.5 White-Red | 1164 | Accelerator Pedal Position 5 Volt Reference (1) (LDE/LXV/2H0)
0.5 White-Red | 1164 | Accelerator Pedal Position 5 Volt Reference (1) (LLW)
0.5 White-Red | 1164 | Accelerator Pedal Position 5 Volt Reference (1) (LXT -SAE)
67 | 0.5 White-Violet | 5905 | Key Capture/Column Lock Shift Position Signal (ATH)
68 | 0.5 Green-Brown | 2087 | Combined Vehicle Inertial Sensor Supply Voltage (FX3)
69 | 0.5 Blue-Yellow | 6795 | Lift Glass/Trunk Motor Release Control 2
70 | 0.5 Violet-White | 239 | Ignition Voltage
71 | 0.5 Violet-White | 239 | Ignition Voltage
0.5 Violet-White | 39 | Ignition Voltage
72 | 0.5 Gray-Green | 328 | Interior Lamp Defeat Switch Signal
73 | 0.5 Yellow | 5191 | Noise Reduction Microphone Active Signal
74 | 0.5 BARE | 5193 | Noise Reduction Microphone Screen
78 | 0.5 Brown-White | 5043 | Keyword 2000 Serial Data
79 | 0.5 Brown-White | 419 | Check Engine Indicator Control
80 | 0.5 Dark Blue | 507 | Wait To Start Indicator Control
0.5 Dark Blue | 507 | Wait To Start Indicator Control (LLW)
81 | 0.5 Blue-Yellow | 6105 | High Speed GMLAN Serial Data (+) (2)
82 | 0.5 White | 6106 | High Speed GMLAN Serial Data (-) (2)
83 | 0.5 Violet-Green | 239 | Ignition Voltage
84 | 0.5 Red-Brown | 3 | Ignition Voltage
0.5 Violet-Black | 3 | Ignition Voltage
0.5 Violet-Black | 3 | Ignition Voltage (ATH)
0.5 Violet-Black | 3 | Ignition Voltage (-ATH)
85 | 0.5 Gray | 1903 | AAS Wheel Speed Sensor Signal Left Front
0.5 Gray | 1903 | AAS Wheel Speed Sensor Signal Left Front (UDK)
87 | 0.5 Blue | 2500 | High Speed GMLAN Serial Data (+) (1)
88 | 0.5 White | 2501 | High Speed GMLAN Serial Data (-) (1)
89 | 10 Red-Yellow | 40 | Battery Positive Voltage
90 | 10 Red-Green | 40 | Battery Positive Voltage
91 | 1.5 Red-Brown | 702 | Battery Positive Voltage (LHD)
1.5 Red-Brown | 702 | Battery Positive Voltage (RHD)
1.5 Red-Brown | 702 | Battery Positive Voltage (LHD ADS)
1.5 Red-Brown | 702 | Battery Positive Voltage (RHD ADS)

Figure 10:

#### X200 Body Harness & Instrument Panel Harness

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 102-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X200 Body Harness & Instrument Panel Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.75 Blue-Yellow | 1960 | Front Center Speaker (-) (UQG)
2 | 0.75 Yellow-White | 1860 | Front Center Speaker (+) (UQG)
8 | 0.5 Brown-Black | 3552 | Passive Start Interior Antenna 1 Signal Hi
9 | 0.5 Blue | 3554 | Passive Start Interior Antenna 2 Signal Hi
10 | 0.5 Gray-Black | 3555 | Passive Start Interior Antenna 2 Signal Lo
11 | 0.5 White | 3553 | Passive Start Interior Antenna 1 Signal Lo
12 | 0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (LHD UQG)
0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (RHD UQG)
13 | 0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (LHD UQG)
0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (RHD UQG)
14 | 0.75 Green-Black | 116 | Left Rear Speaker Signal (-) (LHD UQG)
0.75 Green-Black | 116 | Left Rear Speaker Signal (-) (RHD UQG)
15 | 0.75 Blue-Black | 115 | Right Rear Speaker Signal (-) (LHD UQG)
0.75 Blue-Black | 115 | Right Rear Speaker Signal (-) (RHD UQG)
16 | 0.5 Violet-Black | 7553 | Park Lock Solenoid Control
17 | 0.5 Violet-Black | 3 | Ignition Voltage (ATH)
19 | 0.5 Blue-Yellow | 6105 | High Speed GMLAN Serial Data (+) (2)
20 | 0.5 White | 6106 | High Speed GMLAN Serial Data (-) (2)
21 | 0.5 Red-White | 40 | Battery Positive Voltage
22 | 0.5 Yellow | 40 | Battery Positive Voltage
23 | 0.75 Blue | 201 | Left Front Speaker (+) (1) (LHD UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (RHD UQG)
24 | 0.75 Yellow | 200 | Right Front Speaker (+) (1) (LHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (RHD UQG)
25 | 0.75 Green | 199 | Left Rear Speaker (+) (LHD UQG)
0.75 Green | 199 | Left Rear Speaker (+) (RHD UQG)
26 | 0.75 White | 46 | Right Rear Speaker (+) (LHD UQG)
0.75 White | 46 | Right Rear Speaker (+) (RHD UQG)
27 | 1 Blue-Violet | 807 | OFF /Accessory Voltage
1 Blue-Violet | 807 | OFF /Accessory Voltage (-ATH)
28 | 0.5 Violet-Yellow | 4 | Ignition Voltage (ATH)
29 | 0.5 Black-Gray | 6110 | Clutch Apply Sensor Low Reference
30 | 0.5 Yellow | 6111 | Clutch Apply Sensor Signal
31 | 0.5 Gray-Red | 6109 | Clutch Apply Sensor Voltage Reference
32 | 0.5 Yellow | 7546 | Logistics Relay Control
0.5 Yellow | 7546 | Logistics Relay Control (UAG/UFD)
0.5 Yellow | 7546 | Logistics Relay Control (UDK)
33 | 0.35 Gray-Green | 7565 | Windscreen Temp Sensor Signal (CJ2)
34 | 0.5 Red-Brown | 40 | Battery Positive Voltage
0.5 Red-Violet | 40 | Battery Positive Voltage (ATH)
35 | 0.5 Dark Green | 5103 | Technology Identification
0.5 Green-Black | 5103 | Technology Identification
0.5 Green-Black | 5103 | Technology Identification (UAG/UFD)
0.5 Green-Black | 5103 | Technology Identification (UDK)
36 | 0.5 Yellow-Green | 3274 | Remote Function Actuator Transmit Signal
37 | 0.5 Blue-White | 3275 | Remote Function Actuator Receive Signal
38 | 0.5 Gray-White | 3272 | Remote Function Actuator Supply Voltage
39 | 0.5 Gray | 3273 | Remote Function Actuator Return
40 | 0.75 Green-Violet | 1601 | Steering Column Lock Signal
41 | 0.5 Blue-Gray | 636 | Outside Ambient Air Temperature Sensor Signal
42 | 0.5 Green-Black | 3358 | Left TV Audio Return (ATH)
0.5 Green-Black | 3558 | Passive Start Switch Signal 2 (ATH)
43 | 0.5 Black-Gray | 3359 | Right TV Audio Return (ATH)
0.5 Black-Gray | 3559 | Passive Start Switch 2 Low Reference (ATH)
44 | 0.35 Yellow-Blue | 3197 | Humidity Temperature Sensor Signal (CJ2)
45 | 0.5 Yellow-White | 1161 | Accelerator Pedal Position Signal (1) (LDE/LXV/2H0)
0.5 Yellow-White | 1161 | Accelerator Pedal Position Signal (1) (LLW)
0.5 Yellow-White | 1161 | Accelerator Pedal Position Signal (1) (LXT -SAE)
46 | 0.5 Black-Blue | 1271 | Accelerator Pedal Position Low Reference (1) (LDE/LXV/2H0)
0.5 Black-Blue | 1271 | Accelerator Pedal Position Low Reference (1) (LLW)
0.5 Black-Blue | 1271 | Accelerator Pedal Position Low Reference (1) (LXT -SAE)
47 | 0.5 Black-Violet | 1272 | Accelerator Pedal Position Low Reference (2) (LDE/LXV/2H0)
0.5 Black-Violet | 1272 | Accelerator Pedal Position Low Reference (2) (LLW)
0.5 Black-Violet | 1272 | Accelerator Pedal Position Low Reference (2) (LXT -SAE)
48 | 0.5 Green-White | 1162 | Accelerator Pedal Position Signal (2) (LDE/LXV/2H0)
0.5 Green-White | 1162 | Accelerator Pedal Position Signal (2) (LLW)
0.5 Green-White | 1162 | Accelerator Pedal Position Signal (2) (LXT -SAE)
49 | 0.5 Black-Blue | 61 | Outside Ambient Temperature Sensor Low Reference
50 | 0.5 Violet-White | 5203 | Air Quality Sensor Signal
51 | 0.5 Green-Gray | 6135 | Linear Interconnect Network Bus 4
52 | 0.5 Violet-Green | 39 | Ignition Voltage
53 | 0.5 Violet-Green | 39 | Ignition Voltage
0.5 Violet-Green | 3039 | Run/Crank Ignition 1 Voltage
54 | 0.5 Red-Green | 40 | Battery Positive Voltage
55 | 0.5 Red-Blue | 840 | Battery Positive Voltage
57 | 0.5 Brown-Yellow | 39 | Ignition Voltage
0.5 Brown-Yellow | 239 | Ignition Voltage
58 | 0.75 Gray-Yellow | 6188 | Lift Glass/Trunk Motor Release Control
59 | 0.5 White-Brown | 6815 | Inadvertent Power Control (GLV)
60 | 0.5 Brown-Yellow | 189 | Headlamp Leveling Motor Control
61 | 0.5 Brown-Violet | 193 | Rear Defog Relay Control
62 | - - | - | - (CJ2)
0.35 Dark Green | 50 | Ground
63 | 0.35 Gray-Blue | 7564 | Humidity Sensor Signal (CJ2)
64 | 0.35 Yellow-Red | 597 | 5 Volt Reference (CJ2)
65 | 0.5 Brown-Red | 1274 | Accelerator Pedal Position 5 Volt Reference (2) (LDE/LXV/2H0)
0.5 Brown-Red | 1274 | Accelerator Pedal Position 5 Volt Reference (2) (LLW)
0.5 Brown-Red | 1274 | Accelerator Pedal Position 5 Volt Reference (2) (LXT -SAE)
66 | 0.5 White-Red | 1164 | Accelerator Pedal Position 5 Volt Reference (1) (LDE/LXV/2H0)
0.5 White-Red | 1164 | Accelerator Pedal Position 5 Volt Reference (1) (LLW)
0.5 White-Red | 1164 | Accelerator Pedal Position 5 Volt Reference (1) (LXT -SAE)
67 | 0.5 White-Violet | 5905 | Key Capture/Column Lock Shift Position Signal
68 | 0.5 Green-Brown | 2087 | Combined Vehicle Inertial Sensor Supply Voltage (FX3)
69 | 0.5 Blue-Yellow | 6795 | Lift Glass/Trunk Motor Release Control 2
70 | 0.5 Violet-White | 239 | Ignition Voltage
71 | 0.5 Violet-White | 239 | Ignition Voltage
0.5 Violet-White | 39 | Ignition Voltage
72 | 0.5 Gray-Green | 328 | Interior Lamp Defeat Switch Signal
73 | 0.5 Yellow | 5191 | Noise Reduction Microphone Active Signal
74 | 0.5 BARE | 5193 | Noise Reduction Microphone Screen
78 | 0.5 Brown-White | 5043 | Keyword 2000 Serial Data
79 | 0.5 Brown-White | 419 | Check Engine Indicator Control
80 | 0.5 Dark Blue | 507 | Wait To Start Indicator Control
0.5 Dark Blue | 507 | Wait To Start Indicator Control (LLW)
81 | 0.5 Blue-Yellow | 6105 | High Speed GMLAN Serial Data (+) (2)
82 | 0.5 White | 6106 | High Speed GMLAN Serial Data (-) (2)
83 | 0.5 Violet-Green | 239 | Ignition Voltage
84 | 0.5 Violet-Black | 3 | Ignition Voltage
0.5 Violet-Black | 3 | Ignition Voltage (ATH)
0.5 Violet-Black | 3 | Ignition Voltage (-ATH)
85 | 0.5 Gray | 1903 | AAS Wheel Speed Sensor Signal Left Front
0.5 Gray | 1903 | AAS Wheel Speed Sensor Signal Left Front (UDK)
87 | 0.5 Blue | 2500 | High Speed GMLAN Serial Data (+) (1) (JL9)
0.5 Blue | 2500 | High Speed GMLAN Serial Data (+) (1) (JL9 -SAE)
0.5 Blue | 2500 | High Speed GMLAN Serial Data (+) (1) (SAE)
88 | 0.5 White | 2501 | High Speed GMLAN Serial Data (-) (1) (JL9)
0.5 White | 2501 | High Speed GMLAN Serial Data (-) (1) (JL9 -SAE)
0.5 White | 2501 | High Speed GMLAN Serial Data (-) (1) (SAE)
89 | 10 Red-Yellow | 40 | Battery Positive Voltage
90 | 10 Red-Green | 40 | Battery Positive Voltage
91 | 1.5 Red-Brown | 702 | Battery Positive Voltage
1.5 Red-Brown | 702 | Battery Positive Voltage (LHD ADS)
1.5 Red-Brown | 702 | Battery Positive Voltage (RHD ADS)

Figure 11:

#### X205 Body Harness & Instrument Panel Harness

#### Connector Part Information

- Harness: Instrument panel Instrument panel
- OEM: -
- Service: -
- Description: 12-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X205 Body Harness & Instrument Panel Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 Blue-Black | 1946 | Right Rear Low Level Audio (-)
2 | 0.35 BARE | 2099 | Left Rear Audio Drain Wire
3 | 0.35 Blue-Brown | 1546 | Front Low Level Audio (-)
4 | 0.35 Brown-Violet | 1999 | Left Rear Low Level Audio (-)
5 | 0.5 Violet-Blue | 6978 | Amplifier Control (UQG)
6 | 0.35 Yellow | 512 | Right Front Low Level Audio Signal
7 | 0.35 Brown-White | 546 | Right Rear Low Level Audio Signal
8 | 0.5 Green-Yellow | 7066 | Entertainment Remote Enable Signal (UQG)
9 | 0.35 Brown-Blue | 1947 | Left Front Low Level Audio (-)
10 | 0.35 Green-Black | 599 | Left Rear Low Level Audio Signal
11 | 0.35 BARE | 2011 | Left Front Audio Drain Wire
12 | 0.35 Blue | 511 | Left Front Low Level Audio Signal

Figure 12:

#### X205 Body Harness & Instrument Panel Harness

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 12-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X205 Body Harness & Instrument Panel Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 Blue-Black | 1946 | Right Rear Low Level Audio (-)
2 | 0.35 BARE | 2099 | Left Rear Audio Drain Wire
3 | 0.35 Blue-Brown | 1546 | Front Low Level Audio (-)
4 | 0.35 Brown-Violet | 1999 | Left Rear Low Level Audio (-)
5 | 0.5 Violet-Blue | 6978 | Amplifier Control
6 | 0.35 Yellow | 512 | Right Front Low Level Audio Signal
7 | 0.35 Brown-White | 546 | Right Rear Low Level Audio Signal
8 | 0.5 Green-Yellow | 7066 | Entertainment Remote Enable Signal
9 | 0.35 Brown-Blue | 1947 | Left Front Low Level Audio (-)
10 | 0.35 Green-Black | 599 | Left Rear Low Level Audio Signal
11 | 0.35 BARE | 2011 | Left Front Audio Drain Wire
12 | 0.35 Blue | 511 | Left Front Low Level Audio Signal

Figure 13:

#### X300 Instrument Panel Harness & Console Harness

#### Connector Part Information

- Harness: Console
- OEM: -
- Service: -
- Description: 22-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X300 Instrument Panel Harness & Console Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 Brown | 3345 | Hands Free Kit Jack Common Serial Data
2 | 0.5 White | 3346 | Hands Free Kit Telephone Jack TX Serial Data
3 | 0.5 Gray | 3347 | Hands Free Kit Telephone Jack RX Serial Data
4 | 1 Black | 50 | Ground
5 | 1 Violet | 801 | Retained Accessory Power Fuse Supply Voltage
6 | 0.5 Blue | 3554 | Passive Start Interior Antenna 2 Signal Hi
8 | 0.5 Black | 50 | Ground
9 | 0.5 Green | 3348 | Hands Free Kit Headphone Jack TX Serial Data
10 | 0.5 Blue | 3349 | Hands Free Kit Headphone Jack RX Serial Data
11 | 0.5 Green-Gray | 3277 | Vehicle Anti-Theft System Immobilizer Return (ATH)
12 | 0.35 Green | 5841 | Right Auxiliary Audio Signal (2)
13 | 0.35 Violet | 5843 | Auxiliary Audio Common Signal
14 | 0.35 Gray | 5839 | Left Auxiliary Audio Signal (2)
15 | 0.5 Green-Violet | 7533 | Linear Interconnect Network Bus 11 (ATH)
16 | 0.5 Blue-Violet | 1788 | Traction Control Switch Signal (1)
17 | 0.5 Gray-Black | 3276 | Vehicle Anti-Theft System Immobilizer Supply Voltage (ATH)
18 | 1 Black | 50 | Ground
19 | 1 Violet | 801 | Retained Accessory Power Fuse Supply Voltage
20 | 0.5 Gray-Black | 3555 | Passive Start Interior Antenna 2 Signal Lo
21 | 0.35 BARE | 5842 | Auxiliary Audio Screen (2)
22 | 0.35 Blue | 2060 | Auxiliary Detection Signal

Figure 14:

#### X310 Body Harness & Driver Seat Harness (LHD)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 48-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X310 Body Harness & Driver Seat Harness (LHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.5 Black | 50 | Ground
2 | 2.5 Black | 50 | Ground
3 | 1 Black-Blue | 2433 | Passenger Heated Back Element Return
7 | 0.5 Black-Orange | 1363 | Driver Seat Belt Switch Low Reference
8 | 0.5 Orange-Brown | 238 | Driver Seat Belt Switch Signal
28 | 0.5 Yellow-Orange | 2138 | Left Front Side Impact Module Low Control
30 | 0.5 Orange-Blue | 2137 | Left Front Side Impact Module High Control
43 | 0.5 Green | 5060 | Low Speed GMLAN Serial Data
44 | 0.5 Black-Gray | 2435 | Passenger Heated Seat NTC Low Reference
45 | 0.5 White-Gray | 2434 | Passenger Heated Seat NTC Signal
46 | 1 Brown-Blue | 2479 | Passenger Heated Seat Element Control
47 | 2.5 Red-Green | 40 | Battery Positive Voltage
2.5 Red-White | 40 | Battery Positive Voltage
48 | 1.5 Red-Brown | 702 | Battery Positive Voltage
1.5 Red-Brown | 702 | Battery Positive Voltage (LHD ADS)

Figure 15:

#### X310 Body Harness & Driver Seat Harness (RHD)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 48-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X310 Body Harness & Driver Seat Harness (RHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.5 Black | 50 | Ground
2 | 2.5 Black | 50 | Ground
3 | 1 Black-Blue | 2433 | Passenger Heated Back Element Return
7 | 0.5 Black-Orange | 1363 | Driver Seat Belt Switch Low Reference
8 | 0.5 Orange-Brown | 238 | Driver Seat Belt Switch Signal
28 | 0.5 Yellow-Orange | 2138 | Left Front Side Impact Module Low Control
30 | 0.5 Orange-Blue | 2137 | Left Front Side Impact Module High Control
43 | 0.5 Green | 5060 | Low Speed GMLAN Serial Data
44 | 0.5 Black-Gray | 2435 | Passenger Heated Seat NTC Low Reference
45 | 0.5 White-Gray | 2434 | Passenger Heated Seat NTC Signal
46 | 1 Brown-Blue | 2479 | Passenger Heated Seat Element Control
47 | 2.5 Red-Green | 40 | Battery Positive Voltage
2.5 Red-White | 40 | Battery Positive Voltage
48 | 1.5 Red-Brown | 702 | Battery Positive Voltage
1.5 Red-Brown | 702 | Battery Positive Voltage (RHD ADS)

Figure 16:

#### X315 Body Harness & Front Passenger Seat Harness (LHD)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 48-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X315 Body Harness & Front Passenger Seat Harness (LHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
7 | 0.5 Black-Orange | 1361 | Passenger Seat Belt Switch Low Reference
8 | 0.5 Orange-Violet | 1362 | Passenger Seat Belt Switch Signal
13 | 0.5 Orange-Brown | 7571 | Passenger Seat Belt Reminder Signal
16 | 0.5 Red-Gray | 402 | Battery Positive Voltage
0.5 Red-Gray | 402 | Battery Positive Voltage (AL0)
17 | 0.5 Green | 5060 | Low Speed GMLAN Serial Data
18 | 0.5 Black | 50 | Ground
28 | 0.5 Green-Orange | 2136 | Right Front Side Impact Module Low Control
30 | 0.5 Orange-Yellow | 2135 | Right Front Side Impact Module High Control
44 | 0.5 Black-Gray | 2435 | Passenger Heated Seat NTC Low Reference
45 | 0.5 White-Gray | 2434 | Passenger Heated Seat NTC Signal
46 | 1 Black-Blue | 2433 | Passenger Heated Back Element Return
47 | 1 Brown-Blue | 2479 | Passenger Heated Seat Element Control

Figure 17:

#### X315 Body Harness & Front Passenger Seat Harness (RHD)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 48-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X315 Body Harness & Front Passenger Seat Harness (RHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
7 | 0.5 Black-Orange | 1361 | Passenger Seat Belt Switch Low Reference
8 | 0.5 Orange-Violet | 1362 | Passenger Seat Belt Switch Signal
13 | 0.5 Orange-Brown | 7571 | Passenger Seat Belt Reminder Signal
16 | 0.5 Red-Gray | 402 | Battery Positive Voltage
0.5 Red-Gray | 402 | Battery Positive Voltage (AL0)
17 | 0.5 Green | 5060 | Low Speed GMLAN Serial Data
18 | 0.5 Black | 50 | Ground
28 | 0.5 Green-Orange | 2136 | Right Front Side Impact Module Low Control
30 | 0.5 Orange-Yellow | 2135 | Right Front Side Impact Module High Control
44 | 0.5 Black-Gray | 2435 | Passenger Heated Seat NTC Low Reference
45 | 0.5 White-Gray | 2434 | Passenger Heated Seat NTC Signal
46 | 1 Black-Blue | 2433 | Passenger Heated Back Element Return
47 | 1 Brown-Blue | 2479 | Passenger Heated Seat Element Control

Figure 18:

#### X320 Body Harness & Curtain Airbag Harness

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 2-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X320 Body Harness & Curtain Airbag Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 Orange-Green | 5019 | Left Front Head Curtain Module High Control
B | 0.5 Violet-Orange | 5020 | Left Front Head Curtain Module Low Control

Figure 19:

#### X320 Body Harness & Curtain Airbag Harness

#### Connector Part Information

- Harness: Cable Harness - Curtain Airbag
- OEM: -
- Service: -
- Description: 2-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X320 Body Harness & Curtain Airbag Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 20:

#### X321 Body Harness & Curtain Airbag Harness

#### Connector Part Information

- Harness: Cable Harness - Curtain Airbag
- OEM: -
- Service: -
- Description: 2-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X321 Body Harness & Curtain Airbag Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 21:

#### X401 Body Harness & Fuel Tank Harness

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 16-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X401 Body Harness & Fuel Tank Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | --
2.5 Gray | 120 | Fuel Pump Control (LDE/LXV/2H0)
2.5 Gray | 120 | Fuel Pump Control (SAE LDE OR LXV OR 2H0)
2.5 Gray | 120 | Fuel Pump Control (LLW SAE)
2.5 Gray | 120 | Fuel Pump Control (LLW -SAE)
2.5 Gray | 120 | Fuel Pump Control (LXT SAE)
2.5 Gray | 120 | Fuel Pump Control (LXT -SAE)
B | 0.5 Blue-Violet | 1589 | Primary Fuel Level Sensor Signal
D | 0.5 Yellow-Red | 2709 | Fuel Tank Pressure Sensor 5 Volt Reference (LDE/LXV/2H0)
E | 0.5 White-Brown | 508 | Water In Fuel Indicator Control (LLW)
0.5 Blue-White | 890 | Fuel Tank Pressure Sensor Signal (LDE/LXV/2H0)
F | 0.5 Black-Green | 6281 | Fuel Level Sensor Low Reference (LDE/LXV/2H0)
H | 0.5 Brown-Red | 7445 | Fuel Line Pressure Sensor 5V Reference (SAE LDE OR LXV OR 2H0)
0.5 Brown-Red | 7445 | Fuel Line Pressure Sensor 5V Reference (LLW SAE)
0.5 Brown-Red | 7445 | Fuel Line Pressure Sensor 5V Reference (LXT SAE)
2.5 Red-Blue | 1842 | Battery Positive Voltage
2.5 Red-Blue | 1842 | Battery Positive Voltage (LLW)
J | 2.5 Black | 50 | Ground
2.5 Black | 50 | Ground (LLW)
K | 0.5 Blue-White | 7446 | Fuel Line Pressure Sensor Signal (SAE LDE OR LXV OR 2H0)
0.5 Blue-White | 7446 | Fuel Line Pressure Sensor Signal (LLW SAE)
0.5 Blue-White | 7446 | Fuel Line Pressure Sensor Signal (LXT SAE)
0.5 Yellow-Blue | 1578 | Fuel Temperature Signal (LLW)
L | 0.5 Black-Yellow | 7447 | Fuel Line Pressure Sensor Low Reference (SAE LDE OR LXV OR 2H0)
0.5 Black-Yellow | 7447 | Fuel Line Pressure Sensor Low Reference (LLW SAE)
0.5 Black-Yellow | 7447 | Fuel Line Pressure Sensor Low Reference (LXT SAE)
0.5 Black-Brown | 6062 | Fuel Temperature Sensor Low Reference (LLW)
M | 0.75 Blue | 5372 | Canister Valve Solenoid (LDE/LXV/2H0)
0.75 Blue | 5372 | Canister Valve Solenoid
0.5 Violet-Blue | 5290 | Powertrain Main Relay Fused Supply (1) (LLW)
0.5 Violet-Blue | 5290 | Powertrain Main Relay Fused Supply (1) (LLW)
N | 0.75 White | 1310 | EVAP Canister Vent Solenoid Control (LDE/LXV/2H0)
0.5 Black | 50 | Ground
0.5 Black | 50 | Ground (LLW)
R | 0.5 Black-Green | 6281 | Fuel Level Sensor Low Reference
S | 2 Black | 50 | Ground (LXT -SAE)
2.5 Black | 50 | Ground (LLW -SAE)
2.5 Black | 50 | Ground
2.5 Black | 50 | Ground (LDE/LXV/2H0)
2.5 Black-Green | 1580 | Fuel Pump Low Reference (SAE LDE OR LXV OR 2H0)
2.5 Black-Green | 1580 | Fuel Pump Low Reference (LLW SAE)
2.5 Black-Green | 1580 | Fuel Pump Low Reference (LXT SAE)

Figure 22:

#### X402 Body Harness & Park Pilot Harness (Female)

#### Connector Part Information

- Harness: Rear Panelling
- OEM: -
- Service: -
- Description: 12-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X402 Body Harness & Park Pilot Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 Yellow-Violet | 2378 | Right Rear Corner Object Sensor Signal
B | 0.5 Yellow-White | 2377 | Right Rear Middle Object Sensor Signal
C | 0.5 Yellow-Blue | 2376 | Left Rear Middle Object Sensor Signal
D | - - | - | -
E | 0.5 Yellow | 2375 | Left Rear Corner Object Sensor Signal
F | - - | - | -

Figure 23:

#### X402 Body Harness & Park Pilot Harness

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 12-Way Male (Black/Violet)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X402 Body Harness & Park Pilot Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 Yellow-Violet | 2378 | Right Rear Corner Object Sensor Signal
B | 0.5 Yellow-White | 2377 | Right Rear Middle Object Sensor Signal
C | 0.5 Yellow-Blue | 2376 | Left Rear Middle Object Sensor Signal
D | 0.5 Brown-White | 2374 | Object Sensor Control
E | 0.5 Yellow | 2375 | Left Rear Corner Object Sensor Signal
F | 0.5 Black-Gray | 2379 | Object Sensor Low Reference

Figure 24:

#### X500 Body Harness & Driver Door Harness

#### Connector Part Information

- Harness: Driver Door Harness
- OEM: -
- Service: -
- Description: 41-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X500 Body Harness & Driver Door Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.5 Red-Green | 1540 | Battery Positive Voltage (AEC)
2.5 Red-Green | 1540 | Battery Positive Voltage (AXG)
2.5 Red-Green | 40 | Battery Positive Voltage (AEC)
2.5 Red-Green | 40 | Battery Positive Voltage (AXG)
2 | 2.5 Black | 50 | Ground (AEC)
2.5 Black | 50 | Ground (AXG)
3 | 1.25 Black | 50 | Ground
4 | 0.5 Red-Green | 40 | Battery Positive Voltage
0.5 Red-Green | 40 | Battery Positive Voltage (AXG)
8 | 0.5 Black | 50 | Ground (ATH)
9 | 0.75 Gray | 295 | Door Lock Actuator Lock Control ( -AF8)
0.75 Gray | 295 | Door Lock Actuator Lock Control ( AF8-SAE)
10 | 0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( -AF8)
0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( AF8-SAE)
11 | 0.75 Brown | 5910 | Door Double Lock Actuator Lock Control ( AF8-SAE)
12 | 0.5 Black | 50 | Ground
13 | 0.5 Dark Blue | 6189 | Lift Glass/Trunk Interior Release Signal
14 | 0.75 Blue | 201 | Left Front Speaker (+) (1) (LHD UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (LHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (RHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (RHD UQG)
15 | 0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (RHD UQG)
0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (RHD UQG)
0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (LHD UQG)
0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (LHD UQG)
16 | 0.5 Green-White | 6655 | Driver Door Unlatch Switch Signal
18 | 0.5 Green-Yellow | 6134 | Linear Interconnect Network Bus 3 (AED)
0.5 Green-Yellow | 6134 | Linear Interconnect Network Bus 3 (AXG)
19 | 0.5 Violet-Yellow | 3409 | Mirror Motor Fold Out Control
20 | 0.5 White-Brown | 3410 | Mirror Motor Fold In Control
21 | 0.5 Yellow | 6817 | LED Backlight Dimming Control
22 | 0.5 Green-Black | 3396 | Co-Driver Mirror Motor Right (+) Left (-) Control
23 | 0.5 White | 3398 | Co-Driver Mirror Motor Common Control
24 | 0.5 Yellow-Violet | 3397 | Co-Driver Mirror Motor Up (+) Down (-) Control
25 | 0.75 Black | 50 | Ground (LHD)
0.75 Black | 50 | Ground (RHD)
26 | 0.5 Red-Gray | 40 | Battery Positive Voltage
27 | 0.5 Gray | 745 | Left Front Door Ajar Switch Signal (-AED/-AXG)
28 | 0.5 Brown-Yellow | 2267 | Mirror Heating Element Control
31 | 0.5 Green-White | 3570 | Driver Door Handle Switch Signal
32 | 0.75 Gray | 3578 | Driver Door Unlatch Motor Unlatch Return (ATH)
33 | 0.5 Violet-Gray | 3561 | Passive Entry Driver Door Antenna Signal Lo
34 | 0.5 Violet | 3560 | Passive Entry Driver Door Antenna Signal Hi
40 | 0.5 White-Yellow | 3574 | Driver Door Open Switch Signal (ATH)
41 | 0.75 Violet-Blue | 6666 | Driver Door Unlatch Motor Unlatch Control (ATH)

Figure 25:

#### X500 Body Harness & Driver Door Harness (LHD)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 41-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X500 Body Harness & Driver Door Harness (LHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.5 Red-Green | 40 | Battery Positive Voltage (AEC)
2.5 Red-Green | 40 | Battery Positive Voltage (AXG)
2.5 Red-Green | 1540 | Battery Positive Voltage
2 | 2.5 Black | 50 | Ground
3 | 1 Black | 50 | Ground
4 | 0.5 Red-Green | 40 | Battery Positive Voltage
0.5 Red-Green | 40 | Battery Positive Voltage (AXG)
8 | 0.5 Black | 50 | Ground
9 | 0.75 Gray | 295 | Door Lock Actuator Lock Control ( -AF8)
0.75 Gray | 295 | Door Lock Actuator Lock Control ( AF8-SAE)
10 | 0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( -AF8)
0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( AF8-SAE)
11 | 0.75 Brown | 5910 | Door Double Lock Actuator Lock Control ( AF8-SAE)
12 | 0.5 Black | 50 | Ground
13 | 0.5 Dark Blue | 6189 | Lift Glass/Trunk Interior Release Signal
14 | 0.75 Blue | 201 | Left Front Speaker (+) (1) (LHD UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (LHD 6SP UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (LHD UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (LHD 6SP UQG)
15 | 0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (LHD UQG)
0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (LHD UQG)
16 | 0.5 Green-White | 6655 | Driver Door Unlatch Switch Signal
18 | 0.5 Green-Yellow | 6134 | Linear Interconnect Network Bus 3
19 | 0.5 Violet-Yellow | 3409 | Mirror Motor Fold Out Control
20 | 0.5 White-Brown | 3410 | Mirror Motor Fold In Control
21 | 0.5 Yellow | 6817 | LED Backlight Dimming Control
22 | 0.5 Green-Black | 3396 | Co-Driver Mirror Motor Right (+) Left (-) Control
23 | 0.5 White | 3398 | Co-Driver Mirror Motor Common Control
24 | 0.5 Yellow-Violet | 3397 | Co-Driver Mirror Motor Up (+) Down (-) Control
25 | 0.75 Black | 50 | Ground
26 | - - | - | -
0.5 Red-Gray | 40 | Battery Positive Voltage
27 | 0.5 Gray | 745 | Left Front Door Ajar Switch Signal
28 | 0.5 Brown-Yellow | 2267 | Mirror Heating Element Control
31 | 0.5 Green-White | 3570 | Driver Door Handle Switch Signal
32 | 0.75 Gray | 3578 | Driver Door Unlatch Motor Unlatch Return (ATH)
33 | 0.5 Violet-Gray | 3561 | Passive Entry Driver Door Antenna Signal Lo
34 | 0.5 Violet | 3560 | Passive Entry Driver Door Antenna Signal Hi
40 | 0.5 White-Yellow | 3574 | Driver Door Open Switch Signal (ATH)
41 | 0.75 Violet-Blue | 6666 | Driver Door Unlatch Motor Unlatch Control (ATH)

Figure 26:

#### X500 Body Harness & Driver Door Harness (RHD)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 41-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X500 Body Harness & Driver Door Harness (RHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.5 Red-Green | 40 | Battery Positive Voltage (AEC)
2.5 Red-Green | 40 | Battery Positive Voltage (AXG)
2.5 Red-Green | 1540 | Battery Positive Voltage
2 | 2.5 Black | 50 | Ground
3 | 1 Black | 50 | Ground
4 | 0.5 Red-Green | 40 | Battery Positive Voltage
0.5 Red-Green | 40 | Battery Positive Voltage (AXG)
8 | 0.5 Black | 50 | Ground
9 | 0.75 Gray | 295 | Door Lock Actuator Lock Control ( -AF8)
0.75 Gray | 295 | Door Lock Actuator Lock Control ( AF8-SAE)
10 | 0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( -AF8)
0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( AF8-SAE)
11 | 0.75 Brown | 5910 | Door Double Lock Actuator Lock Control ( AF8-SAE)
12 | 0.5 Black | 50 | Ground
13 | 0.5 Dark Blue | 6189 | Lift Glass/Trunk Interior Release Signal
14 | 0.75 Yellow | 200 | Right Front Speaker (+) (1) (RHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (RHD 6SP UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (RHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (RHD 6SP UQG)
15 | 0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (RHD UQG)
0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (RHD UQG)
16 | 0.5 Green-White | 6655 | Driver Door Unlatch Switch Signal
18 | 0.5 Green-Yellow | 6134 | Linear Interconnect Network Bus 3
19 | 0.5 Violet-Yellow | 3409 | Mirror Motor Fold Out Control
20 | 0.5 White-Brown | 3410 | Mirror Motor Fold In Control
21 | 0.5 Yellow | 6817 | LED Backlight Dimming Control
22 | 0.5 Green-Black | 3396 | Co-Driver Mirror Motor Right (+) Left (-) Control
23 | 0.5 White | 3398 | Co-Driver Mirror Motor Common Control
24 | 0.5 Yellow-Violet | 3397 | Co-Driver Mirror Motor Up (+) Down (-) Control
25 | 0.75 Black | 50 | Ground
26 | - - | - | -
0.5 Red-Gray | 40 | Battery Positive Voltage
27 | 0.5 Gray | 745 | Left Front Door Ajar Switch Signal
28 | 0.5 Brown-Yellow | 2267 | Mirror Heating Element Control
31 | 0.5 Green-White | 3570 | Driver Door Handle Switch Signal
32 | 0.75 Gray | 3578 | Driver Door Unlatch Motor Unlatch Return (ATH)
33 | 0.5 Violet-Gray | 3561 | Passive Entry Driver Door Antenna Signal Lo
34 | 0.5 Violet | 3560 | Passive Entry Driver Door Antenna Signal Hi
40 | 0.5 White-Yellow | 3574 | Driver Door Open Switch Signal (ATH)
41 | 0.75 Violet-Blue | 6666 | Driver Door Unlatch Motor Unlatch Control (ATH)

Figure 27:

#### X50A (X1) Fuse Block - Underhood X1

#### Connector Part Information

- Harness: Forward Lamp
- OEM: -
- Service: -
- Description: 82-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X50A (X1) Fuse Block - Underhood X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
11 | 1 Brown-Gray | 29 | Horn Control
13 | 1.5 White | 311 | Right Headlamp High Beam Control
14 | 1.5 White | 711 | Left Headlamp High Beam Control
20 | 0.5 Red-White | 999 | - (FI)
0.5 Red-White | 999 | - (LXV LDE 2H0)
0.5 Red-White | 999 | - (LXT)
21 | 0.5 Violet-Green | 839 | Run/Crank Ignition 1 Voltage (D)
0.5 Violet-Green | 839 | Run/Crank Ignition 1 Voltage (LLW)
30 | 1 Gray-Violet | 228 | Windshield Washer Pump Control
31 | 0.75 Violet-Brown | 34 | Front Fog Lamp Control
34 | 0.5 Brown-Yellow | 473 | High Speed Cooling Fan Relay Control (D)
2.5 Brown-Yellow | 473 | High Speed Cooling Fan Relay Control (LLW)
2.5 White-Black | 473 | High Speed Cooling Fan Relay Control (FI)
2.5 White-Black | 2366 | Cooling Fan Control Relay Speed Signal (FI)
2.5 White-Black | 2366 | Cooling Fan Control Relay Speed Signal (LXV LDE 2H0)
2.5 White-Black | 2366 | Cooling Fan Control Relay Speed Signal (LXT)
37 | 4 White-Black | 2366 | Cooling Fan Control Relay Speed Signal (LLW)
43 | 2.5 White-Black | 2366 | Cooling Fan Control Relay Speed Signal (FI)
2.5 White-Black | 2366 | Cooling Fan Control Relay Speed Signal (LXV LDE 2H0)
2.5 White-Black | 2366 | Cooling Fan Control Relay Speed Signal (LXT)
2.5 White-Black | 473 | High Speed Cooling Fan Relay Control (FI)
46 | 2.5 Gray | 532 | Cooling Fan Motor Control (2)
2.5 Gray | 532 | Cooling Fan Motor Control (2) (LXV LDE 2H0)
2.5 Gray | 532 | Cooling Fan Motor Control (2) (LLW)
2.5 Gray | 532 | Cooling Fan Motor Control (2) (LXT)
47 | 2.5 White-Blue | 409 | Cooling Fan Motor Control (1) (FI)
2.5 White-Blue | 409 | Cooling Fan Motor Control (1) (LXV LDE 2H0)
2.5 White-Blue | 409 | Cooling Fan Motor Control (1) (LXT)
50 | 4 Yellow | 5358 | Cooling Fan Motor Control (3)
4 Yellow | 5358 | Cooling Fan Motor Control (3) (LXV LDE 2H0)
4 Yellow | 5358 | Cooling Fan Motor Control (3) (LLW)
4 Yellow | 5358 | Cooling Fan Motor Control (3) (LXT)
52 | 0.5 Red-Gray | 1042 | Battery Positive Voltage (LLW)
53 | 0.5 Brown-Red | 2700 | A/C Pressure Sensor 5 Volt Reference (LDE/LXV/2H0)
0.5 Brown-Red | 2700 | A/C Pressure Sensor 5 Volt Reference (LLW)
0.5 Brown-Red | 2700 | A/C Pressure Sensor 5 Volt Reference (LXT)
54 | 0.5 Black-Blue | 6813 | Coolant Temperature Sensor #2 Low Reference (LDE/LXV/2H0)
55 | 0.5 Black-Brown | 5514 | A/C Refrigerant Pressure Sensor Low Reference (LDE/LXV/2H0)
0.5 Black-Brown | 5514 | A/C Refrigerant Pressure Sensor Low Reference (LLW)
0.5 Black-Brown | 5514 | A/C Refrigerant Pressure Sensor Low Reference (LXT)
56 | 0.5 Green-Violet | 2032 | Coolant Temperature Sensor Signal (LDE/LXV/2H0)
57 | 0.5 Green | 380 | A/C Refrigerant Pressure Sensor Signal (LDE/LXV/2H0)
0.5 Green | 380 | A/C Refrigerant Pressure Sensor Signal (LLW)
0.5 Green | 380 | A/C Refrigerant Pressure Sensor Signal (LXT)
65 | 0.5 Violet-Green | 1339 | Run/Crank Ignition 1 Voltage
0.5 Violet-Green | 39 | Ignition Voltage
66 | 0.5 Red-White | 999 | - (FI)
0.5 Red-White | 999 | - (LXV LDE 2H0)
0.5 Red-White | 999 | - (LXT)
0.5 Violet-Green | 839 | Run/Crank Ignition 1 Voltage (LLW)
0.5 Violet-Green | 839 | Run/Crank Ignition 1 Voltage (D)
67 | 0.5 Green | 7625 | Cooling Fan Motor Supply Voltage (4)
0.5 Green | 7625 | Cooling Fan Motor Supply Voltage (4) (LXV LDE 2H0)
0.5 Green | 7625 | Cooling Fan Motor Supply Voltage (4) (LLW)
0.5 Green | 7625 | Cooling Fan Motor Supply Voltage (4) (LXT)
68 | 0.5 Green | 7625 | Cooling Fan Motor Supply Voltage (4) (LXV LDE 2H0)
0.5 Green | 7625 | Cooling Fan Motor Supply Voltage (4) (LLW)
0.5 Green | 7625 | Cooling Fan Motor Supply Voltage (4) (LXT)
- - | - | -
71 | 2.5 Black | 50 | Ground
72 | 2.5 White | 92 | Windshield Wiper Motor High Speed Control
73 | 2.5 Yellow-Brown | 95 | Windshield Wiper Motor Low Speed Control
74 | 2.5 Black | 50 | Ground

Figure 28:

#### X50A (X2) Fuse Block - Underhood X2

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 74-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X50A (X2) Fuse Block - Underhood X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
4 | 0.75 Gray | 295 | Door Lock Actuator Lock Control (-AF8 SAE)
5 | 0.75 White-Blue | 3266 | Child Security Lock Motor Unlock Control (-AF8 SAE)
6 | 2.5 Gray | 120 | Fuel Pump Control
2.5 Gray | 120 | Fuel Pump Control (LDE/LXV/2H0)
2.5 Gray | 120 | Fuel Pump Control (LLW -SAE)
2.5 Gray | 120 | Fuel Pump Control (LXT -SAE)
10 | 0.75 Brown-Green | 59 | A/C Compressor Clutch Control (LXT)
0.5 Brown-Green | 59 | A/C Compressor Clutch Control (LXT)
12 | 0.75 Gray-Green | 3271 | Door Lock Control (2) ( -AF8 SAE)
13 | 0.75 Violet-Yellow | 3267 | Child Security Lock Relay Control (-AF8 SAE)
14 | 0.5 Violet-Green | 39 | Ignition Voltage
0.5 Violet-Green | 3039 | Run/Crank Ignition 1 Voltage
15 | 0.5 Violet-Pink | 39 | Ignition Voltage (SAE LDE OR LXV OR 2H0)
0.5 Violet-Black | 739 | Run/Crank Ignition 1 Voltage (LLW SAE)
0.5 Violet-Black | 739 | Run/Crank Ignition 1 Voltage
0.5 Violet-Black | 39 | Ignition Voltage (LXT SAE)
16 | 0.5 Violet-Blue | 5290 | Powertrain Main Relay Fused Supply (1) (LLW)
0.5 Violet-Blue | 5290 | Powertrain Main Relay Fused Supply (1) (LLW)
17 | 0.5 Brown-White | 5069 | Engine Main Relay Coil Control (LLW)
0.5 Brown-Violet | 1594 | Ignition 3 Relay Control
0.5 Brown-Violet | 1594 | Ignition 3 Relay Control (ATH)
0.5 Brown-Violet | 1594 | Ignition 3 Relay Control (-ATH)
19 | 0.5 Brown-White | 1317 | Fog Lamp Relay Control
21 | 0.5 Blue-Brown | 7573 | Electric Variable Displacement Supply
0.5 Blue-Brown | 7573 | Electric Variable Displacement Supply (LDE/LXV/2H0)
0.5 Blue-Brown | 7573 | Electric Variable Displacement Supply (LLW)
0.5 Blue-Brown | 7573 | Electric Variable Displacement Supply (LXT)
22 | 0.5 Gray | 91 | Windshield Wiper Motor Relay Coil Control
23 | 0.5 Red-Gray | 40 | Battery Positive Voltage
25 | 0.5 Brown-White | 28 | Horn Relay Control
26 | 0.5 Violet-White | 239 | Ignition Voltage
28 | 0.5 Red-Gray | 40 | Battery Positive Voltage
0.5 Red-Green | 40 | Battery Positive Voltage (AXG)
0.5 Red-Green | 40 | Battery Positive Voltage
29 | 0.5 Violet-White | 39 | Ignition Voltage
0.5 Violet-White | 239 | Ignition Voltage
31 | 0.5 Violet-White | 39 | Ignition Voltage
-- | -- | --
32 | 1 Blue-Violet | 807 | OFF /Accessory Voltage
1 Blue-Violet | 807 | OFF /Accessory Voltage (-ATH)
33 | 4 Red-Brown | 40 | Battery Positive Voltage
4 Red-Brown | 40 | Battery Positive Voltage (AEQ)
36 | 4 Red-Green | 1540 | Battery Positive Voltage
4.0 Red-Green | 40 | Battery Positive Voltage
4 Red-Green | 40 | Battery Positive Voltage (AEC)
2.5 Red-Green | 40 | Battery Positive Voltage (AXG)
37 | 2.5 Red-Blue | 1842 | Battery Positive Voltage
2.5 Red-Blue | 1842 | Battery Positive Voltage (LLW)
39 | 4 Brown-Violet | 293 | Rear Defog Element Control
40 | 2.5 Red-Violet | 40 | Battery Positive Voltage
41 | 4 Red-Violet | 40 | Battery Positive Voltage
42 | 4 Red-Green | 40 | Battery Positive Voltage
4 Red-Green | 40 | Battery Positive Voltage (ATH)
45 | 0.5 White-Violet | 860 | Front Windshield Wiper Switch High Signal
48 | 0.5 Blue-Brown | 7547 | Security Lock Relay Control (AF8-SAE)
49 | 0.5 Brown-Blue | 1977 | Rear Fog Lamp Relay Control
50 | 0.75 Gray | 295 | Door Lock Actuator Lock Control (AF8 AF8-SAE)
51 | 0.5 Yellow-Gray | 122 | Rear Fog Lamp Control
52 | 0.75 Blue-White | 195 | Door Lock Control (AF8 AF8-SAE)
53 | 0.75 Brown | 5910 | Door Double Lock Actuator Lock Control (AF8-SAE)
56 | 1 Red-Green | 40 | Battery Positive Voltage
1.5 Red-Green | 1840 | Battery Positive Voltage
58 | 0.5 Brown-Violet | 1969 | Headlamp High Beam Relay Control
60 | 0.5 Brown-Gray | 2268 | Windshield Washer Relay Control
61 | 0.5 Brown-Violet | 193 | Rear Defog Relay Control
62 | 0.5 Brown-Yellow | 2267 | Mirror Heating Element Control
63 | 0.5 Red-Gray | 402 | Battery Positive Voltage
0.5 Red-Gray | 402 | Battery Positive Voltage (AL0)
64 | 0.5 Red-White | 40 | Battery Positive Voltage
67 | 1.5 Red-White | 40 | Battery Positive Voltage
68 | 1.5 Red-Violet | 40 | Battery Positive Voltage
69 | 2.5 Red-White | 40 | Battery Positive Voltage
2.5 Red-Green | 40 | Battery Positive Voltage
70 | 2.5 Red-White | 40 | Battery Positive Voltage
71 | 2.5 Red-White | 40 | Battery Positive Voltage
2.5 Red-White | 40 | Battery Positive Voltage (UQG)
72 | 0.5 Red-Brown | 40 | Battery Positive Voltage
73 | 0.5 Blue-Brown | 7573 | Electric Variable Displacement Supply
0.5 Blue-Brown | 7573 | Electric Variable Displacement Supply (LDE/LXV/2H0)
0.5 Blue-Brown | 7573 | Electric Variable Displacement Supply (LLW)
0.5 Blue-Brown | 7573 | Electric Variable Displacement Supply (LXT)
74 | 2.5 Red-Gray | 40 | Battery Positive Voltage
2.5 Red-Gray | 40 | Battery Positive Voltage (SAE LDE OR LXV OR 2H0)
2.5 Red-Gray | 40 | Battery Positive Voltage (LLW SAE)
2.5 Red-Gray | 40 | Battery Positive Voltage (LXT SAE)

Figure 29:

#### X50D Fuse Block - Battery X6

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 1-Way (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X50D Fuse Block - Battery X6

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 30:

#### X600 Body Harness & Passenger Door Harness

#### Connector Part Information

- Harness: Cable Harness - Front Passenger door
- OEM: -
- Service: -
- Description: 41-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X600 Body Harness & Passenger Door Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.5 Red-Green | 40 | Battery Positive Voltage
2.5 Red-Green | 1540 | Battery Positive Voltage
2 | 2.5 Black | 50 | Ground
3 | 1 Black | 50 | Ground
5 | 0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( -AF8)
0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( AF8-SAE)
8 | 0.5 Black | 50 | Ground
2 Black | 50 | Ground
9 | 0.75 Gray | 295 | Door Lock Actuator Lock Control ( -AF8)
0.75 Gray | 295 | Door Lock Actuator Lock Control ( AF8-SAE)
10 | 0.75 Brown | 5910 | Door Double Lock Actuator Lock Control ( AF8-SAE)
11 | 0.5 Yellow-Violet | 3397 | Co-Driver Mirror Motor Up (+) Down (-) Control
13 | 0.5 Green-Black | 3396 | Co-Driver Mirror Motor Right (+) Left (-) Control
14 | 0.5 White | 3398 | Co-Driver Mirror Motor Common Control
15 | 0.5 Green-Yellow | 6134 | Linear Interconnect Network Bus 3
16 | 0.75 Gray-Blue | 3576 | Co-Driver Door Exterior Switch Lock Signal
17 | 0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (LHD UQG)
0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (LHD UQG)
0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (RHD UQG)
0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (RHD UQG)
18 | 0.75 Blue | 201 | Left Front Speaker (+) (1) (RHD UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (RHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (LHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (LHD UQG)
21 | 0.5 White-Brown | 3410 | Mirror Motor Fold In Control
22 | 0.5 Violet-Yellow | 3409 | Mirror Motor Fold Out Control
23 | 0.5 Brown-Yellow | 2267 | Mirror Heating Element Control
27 | 0.5 Gray | 746 | Right Front Door Ajar Switch Signal (-AED)
31 | 0.5 Violet-White | 3571 | Co_Driver Door Handle Switch Signal
32 | 0.75 Gray-Black | 3579 | Co Driver Door Unlatch Motor Unlatch Return (ATH)
33 | 0.5 Green-Black | 3563 | Passive Entry Co_Driver Door Antenna Signal Lo
34 | 0.5 Green-Yellow | 3562 | Passive Entry Co_Driver Door Antenna Signal Hi
40 | 0.5 Gray-Green | 3575 | Co_Driver Door Open Switch Signal (ATH)
41 | 0.75 Yellow-Green | 3583 | Co Driver Door Unlatch Motor Unlatch Control (ATH)

Figure 31:

#### X600 Body Harness & Passenger Door Harness (LHD)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 41-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X600 Body Harness & Passenger Door Harness (LHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.5 Red-Green | 40 | Battery Positive Voltage
2.5 Red-Green | 1540 | Battery Positive Voltage
2 | 2 Black | 50 | Ground
3 | 1 Black | 50 | Ground
5 | 0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( -AF8)
0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( AF8-SAE)
8 | 1 Black | 50 | Ground
9 | 0.75 Gray | 295 | Door Lock Actuator Lock Control ( -AF8)
0.75 Gray | 295 | Door Lock Actuator Lock Control ( AF8-SAE)
10 | 0.75 Brown | 5910 | Door Double Lock Actuator Lock Control ( AF8-SAE)
11 | 0.5 Yellow-Violet | 3397 | Co-Driver Mirror Motor Up (+) Down (-) Control
13 | 0.5 Green-Black | 3396 | Co-Driver Mirror Motor Right (+) Left (-) Control
14 | 0.5 White | 3398 | Co-Driver Mirror Motor Common Control
15 | 0.5 Green-Yellow | 6134 | Linear Interconnect Network Bus 3
16 | 0.75 Gray-Blue | 3576 | Co-Driver Door Exterior Switch Lock Signal
17 | 0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (LHD UQG)
0.75 Yellow-Black | 117 | Right Front Speaker Signal (-) (1) (LHD UQG)
18 | 0.75 Yellow | 200 | Right Front Speaker (+) (1) (LHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (LHD 6SP UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (LHD UQG)
0.75 Yellow | 200 | Right Front Speaker (+) (1) (LHD 6SP UQG)
21 | 0.5 White-Brown | 3410 | Mirror Motor Fold In Control
22 | 0.5 Violet-Yellow | 3409 | Mirror Motor Fold Out Control
23 | 0.5 Brown-Yellow | 2267 | Mirror Heating Element Control
27 | 0.5 Gray | 746 | Right Front Door Ajar Switch Signal
31 | 0.5 Violet-White | 3571 | Co_Driver Door Handle Switch Signal
32 | 0.75 Gray-Black | 3579 | Co Driver Door Unlatch Motor Unlatch Return (ATH)
33 | 0.5 Green-Black | 3563 | Passive Entry Co_Driver Door Antenna Signal Lo
34 | 0.5 Green-Yellow | 3562 | Passive Entry Co_Driver Door Antenna Signal Hi
40 | 0.5 Gray-Green | 3575 | Co_Driver Door Open Switch Signal (ATH)
41 | 0.75 Yellow-Green | 3583 | Co Driver Door Unlatch Motor Unlatch Control (ATH)

Figure 32:

#### X600 Body Harness & Passenger Door Harness (RHD)

#### Connector Part Information

- Harness: Body
- OEM: -
- Service: -
- Description: 41-Way Male (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X600 Body Harness & Passenger Door Harness (RHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.5 Red-Green | 40 | Battery Positive Voltage
2.5 Red-Green | 1540 | Battery Positive Voltage
2 | 2 Black | 50 | Ground
3 | 1 Black | 50 | Ground
5 | 0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( -AF8)
0.75 Brown-Yellow | 294 | Door Lock Actuator Unlock Control ( AF8-SAE)
8 | 1 Black | 50 | Ground
9 | 0.75 Gray | 295 | Door Lock Actuator Lock Control ( -AF8)
0.75 Gray | 295 | Door Lock Actuator Lock Control ( AF8-SAE)
10 | 0.75 Brown | 5910 | Door Double Lock Actuator Lock Control ( AF8-SAE)
11 | 0.5 Yellow-Violet | 3397 | Co-Driver Mirror Motor Up (+) Down (-) Control
13 | 0.5 Green-Black | 3396 | Co-Driver Mirror Motor Right (+) Left (-) Control
14 | 0.5 White | 3398 | Co-Driver Mirror Motor Common Control
15 | 0.5 Green-Yellow | 6134 | Linear Interconnect Network Bus 3
16 | 0.75 Gray-Blue | 3576 | Co-Driver Door Exterior Switch Lock Signal
17 | 0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (RHD UQG)
0.75 Brown-Blue | 118 | Left Front Speaker Signal (-) (1) (RHD UQG)
18 | 0.75 Blue | 201 | Left Front Speaker (+) (1) (RHD UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (RHD 6SP UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (RHD UQG)
0.75 Blue | 201 | Left Front Speaker (+) (1) (RHD 6SP UQG)
21 | 0.5 White-Brown | 3410 | Mirror Motor Fold In Control
22 | 0.5 Violet-Yellow | 3409 | Mirror Motor Fold Out Control
23 | 0.5 Brown-Yellow | 2267 | Mirror Heating Element Control
27 | 0.5 Gray | 746 | Right Front Door Ajar Switch Signal
31 | 0.5 Violet-White | 3571 | Co_Driver Door Handle Switch Signal
32 | 0.75 Gray-Black | 3579 | Co Driver Door Unlatch Motor Unlatch Return (ATH)
33 | 0.5 Green-Black | 3563 | Passive Entry Co_Driver Door Antenna Signal Lo
34 | 0.5 Green-Yellow | 3562 | Passive Entry Co_Driver Door Antenna Signal Hi
40 | 0.5 Gray-Green | 3575 | Co_Driver Door Open Switch Signal (ATH)
41 | 0.75 Yellow-Green | 3583 | Co Driver Door Unlatch Motor Unlatch Control (ATH)

Figure 33:

#### X70 Relay Block - Underhood X3

#### Connector Part Information

- Harness: Engine Cooling
- OEM: -
- Service: -
- Description: 9-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X70 Relay Block - Underhood X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
2 | 4 Black | 50 | Ground (LLW)
4 | 0.5 Violet-Green | 839 | Run/Crank Ignition 1 Voltage
0.5 Violet-Green | 839 | Run/Crank Ignition 1 Voltage (LLW)
5 | 4 Black | 50 | Ground
4 Blue-Violet | 2364 | Cooling Fan Speed Signal (LLW)
6 | 0.5 Red-Gray | 1042 | Battery Positive Voltage (LLW)
8 | 4 Black | 50 | Ground (LLW)

Figure 34:

#### X84 Data Link Connector

#### Connector Part Information

- Harness: Instrument Panel
- OEM: -
- Service: -
- Description: 16-Way Female (Black)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X84 Data Link Connector

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 Green | 5060 | Low Speed GMLAN Serial Data
4 | 0.5 Black | 50 | Ground
5 | 0.5 Black | 50 | Ground
6 | 0.5 Blue | 2500 | High Speed GMLAN Serial Data (+) (1)
7 | 0.5 Brown-White | 5043 | Keyword 2000 Serial Data
12 | 0.5 Blue-Yellow | 6105 | High Speed GMLAN Serial Data (+) (2)
13 | 0.5 White | 6106 | High Speed GMLAN Serial Data (-) (2)
14 | 0.5 White | 2501 | High Speed GMLAN Serial Data (-) (1)
16 | 0.5 Red-Blue | 40 | Battery Positive Voltage
0.5 Red-Blue | 840 | Battery Positive Voltage

Figure 35:

#### X85 Steering Wheel Air Bag Coil X1

#### Connector Part Information

- Harness: Instrument Panel
- OEM: 13175269
- Service: -
- Description: 10-Way Female (-)

#### Terminal Part Information

- Pins:
- Terminated Lead:
- Release Tool: J-38125-215A
- Diagnostic Test Probe: J-35616-64B (L-BU)

#### X85 Steering Wheel Air Bag Coil X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 Green-White | 3287 | Horn Switch Signal
2 | 0.5 Black | 50 | Ground
3 | 0.5 Gray-Green | 5737 | Adaptive Cruise Control Gap Up/Down Switch Signal
4 | 0.5 Green-White | 6819 | Steering Wheel Resistor Ladder Signal #2
5 | 0.5 White-Red | 1444 | 12 Volt Reference
6 | 0.5 Yellow | 6817 | LED Backlight Dimming Control

Figure 36:

#### X85 Steering Wheel Air Bag Coil X2

#### Connector Part Information

- Harness: Instrument Panel
- OEM: -
- Service: Service by Connector Assembly
- Description: 4-Way Female (Yellow)

#### Terminal Part Information

- Pins:
- Terminated Lead: Service by Connector Assembly
- Release Tool: 12180559-1
- Diagnostic Test Probe: J-35616-64B (L-BU)

#### X85 Steering Wheel Air Bag Coil X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 Orange-Violet | 3021 | Steering Wheel Module Stage 1 High Control
2 | 0.5 Brown-Orange | 3020 | Steering Wheel Module Stage 1 Low Control
3 | 0.5 Orange-Green | 3023 | Steering Wheel Module Stage 2 High Control
4 | 0.5 White-Orange | 3022 | Steering Wheel Module Stage 2 Low Control

Figure 37:

#### X85 (X3) Steering Wheel Air Bag Coil X3 (Female)

#### Connector Part Information

- OEM:
- Service:
- Description:

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X85 (X3) Steering Wheel Air Bag Coil X3 (Female)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 38:

#### X900 Body Harness & Liftgate Harness

#### Connector Part Information

- Harness: Liftgate
- OEM: -
- Service: -
- Description: 12-Way Female (-)

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X900 Body Harness & Liftgate Harness

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 Blue-Yellow | 6795 | Lift Glass/Trunk Motor Release Control 2
2 | 0.5 Violet-Gray | 1303 | Lift Gate Ajar Switch Signal (1)
4 | 0.5 Green-Yellow | 6846 | Rear License Lamp Control
5 | 0.5 Yellow-Gray | 122 | Rear Fog Lamp Control
6 | 0.5 Black | 50 | Ground
10 | 0.5 Violet-Gray | 709 | Left Park Lamp Control (DOM)
0.5 Violet-Gray | 709 | Left Park Lamp Control (SAE)
11 | 0.5 Gray-Brown | 309 | Right Park Lamp Control (DOM)
0.5 Gray-Brown | 309 | Right Park Lamp Control (SAE)
12 | 0.5 Black | 50 | Ground

Figure 39:

#### X900 Body Harness & Liftgate Harness (Male)

#### Connector Part Information

- OEM:
- Service:
- Description:

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X900 Body Harness & Liftgate Harness (Male)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 40:

#### X912 Body Harness & Tail Lamp Left Harness (Male) (SAE)

#### Connector Part Information

- OEM:
- Service:
- Description:

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X912 Body Harness & Tail Lamp Left Harness (Male) (SAE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 41:

#### X913 Body Harness & Tail Lamp Right Harness (Male) (SAE)

#### Connector Part Information

- OEM:
- Service:
- Description:

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X913 Body Harness & Tail Lamp Right Harness (Male) (SAE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 42:

#### X914 Liftgate Harness & Liftgate Tail Lamp Left Harness (Female) (DOM)

#### Connector Part Information

- OEM:
- Service:
- Description:

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X914 Liftgate Harness & Liftgate Tail Lamp Left Harness (Female) (DOM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 43:

#### X915 Liftgate Harness & Liftgate Tail Lamp Left Harness (Male) (SAE)

#### Connector Part Information

- OEM:
- Service:
- Description:

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X915 Liftgate Harness & Liftgate Tail Lamp Left Harness (Male) (SAE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 44:

#### X917 Liftgate Harness & Liftgate Tail Lamp Right Harness (Male) (SAE)

#### Connector Part Information

- OEM:
- Service:
- Description:

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X917 Liftgate Harness & Liftgate Tail Lamp Right Harness (Male) (SAE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---

Figure 45:

#### X92 (X1) Universal Serial Bus (USB) Connector X1 (Female)

#### Connector Part Information

- OEM:
- Service:
- Description:

#### Terminal Part Information

- Terminal/Tray:
- Core/Insulation Crimp:
- Release Tool/Test Probe:

#### X92 (X1) Universal Serial Bus (USB) Connector X1 (Female)

Pin | Wire | Circuit | Function
--- | --- | --- | ---