For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Exhaust Service Warning in the Preface section. Warning: Refer to Protective Goggles and Glove Warning in the Preface section.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Detach the exhaust system from the Underbody.

1 | Heat Shield Retainer (QTY: 4)
2 | Exhaust Rear Muffler Heat Shield