For 1990-2009 cars

## Fuel Tank Heat Shield Replacement 2L Diesel LLW

Callout | Component Name
--- | ---
Warning: Refer to Safety Goggles and Fuel Warning in the Preface section. Warning: Refer to Actions to Take When Working with Fuel Warning in the Preface section.

#### Preliminary Procedure

Remove the fuel tank. Refer to Fuel Tank Replacement.

1 | Fuel Tank Heat Shield Bolt (Qty: 3)
2 | Fuel Tank Heat Shield

## Fuel Tank Heat Shield Replacement 1.6L LXV

Callout | Component Name
--- | ---
Warning: Refer to Safety Goggles and Fuel Warning in the Preface section. Warning: Refer to Actions to Take When Working with Fuel Warning in the Preface section.

#### Preliminary Procedure

Remove the fuel tank. Refer to Fuel Tank Replacement.

1 | Fuel Tank Heat Shield Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten: 2.5 N·m (23 lb in)
2 | Fuel Tank Heat Shield