For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Side Door Pull Handle Cap Tip Use suitable tool to unsnap.
2 | Front Side Door Pull Handle Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Front Side Door Inside Handle Bolt Finish Cap Tip Pull handle back to remove cap. Use suitable tool to unsnap.
4 | Front Side Door Inside Handle Bolt Tighten 2.5 N·m (22 lb in)
5 | Front Side Door Trim Clip (Qty. 10)
6 | Front Side Door Trim Assembly

#### Procedure

1. Pull upwards on the door lock retainer cable to disengage.
2. Disconnect the electrical connectors.