For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove rear wheelhouse panel liner. Refer to Rear Wheelhouse Panel Liner Replacement.
2. Remove fuel tank filler door. Refer to Fuel Tank Filler Door Replacement.

1 | Fuel Tank Filler Door Lock Actuator

#### Procedure

Disconnect electrical connector.

2 | Fuel Tank Filler Pipe Housing

#### Procedure

Unclip 4 clips and remove.

Note: Push fuel tank filler door lock actuator locking rod in closed position.