For 1990-2009 cars

### Removal Procedure

1. Remove the wheel speed sensor screw (1) from the steering knuckle.
2. Remove wheel speed sensor (2)
3. Remove the wiring harness retainers from the frame.
4. Disconnect the electrical connector.
5. Remove wheel speed sensor (1) from vehicle

### Installation Procedure

1. Install the wheel speed sensor (1) to the vehicle
2. Connect the electical connector.
3. Install the wiring harness retainers to the the frame.
4. Install the wheel speed sensor (2) to steering knuckle.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the wheel speed sensor screw (1) and tighten to 9 N·m (80 lb in).