For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the headlamp. Refer to Headlamp Replacement.
3. Remove the front fender. Refer to Front Fender Replacement.

1 | Front Fender Bracket Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m(80 lb in)
2 | Front Fender Front Lower Bracket