For 1990-2009 cars

Application | Specification
Metric | English
Air Conditioning Compressor Bolt | 22 N·m | 17 lb ft
Air Conditioning Evaporator Hose Assembly Nut to Air Conditioning Compressor and Condenser Hose | 19 N·m | 14 lb ft
Air Conditioning Evaporator Hose Assembly Nut to Air Conditioning Condenser | 19 N·m | 14 lb ft
Air Conditioning Evaporator Hose Assembly Nut to Air Conditioning Evaporator Thermal Expansion Valve | 19 N·m | 14 lb ft
Air Conditioning Compressor Oil Drain Plug | 15 N·m | 11 lb ft
Air Conditioning Control Module Bolt | 2,5 N·m | 23 lb in
Air Conditioning Evaporator Case Bolt | 2,5 N·m | 23 lb in
Air Conditioning Evaporator Thermal Expansion Valve Bolt | 15 N·m | 11 lb ft
Air Conditioning Refrigerant Pressure Sensor | xx N·m | xx lb ft
Air Outlet Duct Bolt | 2,5 N·m | 23 lb in
Auxiliary Heater Core Bolts | xx N·m | xx lb in
Blower Motor Bolt | 4,5 N·m | 40 lb in
Blower Motor Cup Bolt | 2,5 N·m | 23 lb in
Condenser Hose And Condenser Hose Bolt | xx N·m | xx lb in
Floor Air Outlet Duct Bolt | 2,5 N·m | 23 lb in
Heater and Air Conditioning Evaporator Case Bolt | 2,5 N·m | 23 lb in
Heater Core Cover Bolt | 2,5 N·m | 23 lb in
Heater and Blower and Air Conditioning Control Module Bolt | 2,5 N·m | 23 lb in
Instrument Panel Bracket Bolt | 9 N·m | 80 lb in
Instrument Panel Tie Bar Bolt | 22 N·m | 17 lb ft
Instrument Panel Tie Bar Nuts | xx N·m | xx lb ft
Mode Control Cam Actuator Screws | xx N·m | xx lb in
Refrigerant Pressure Sensor | 9 N·m | 80 lb in
Service Valve Core | 3 N·m | 27 lb in
TXV Mounting Bolts | xx N·m | xx lb ft