For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector (1) from the speedometer driven gear (2).
2. Remove the speedometer bolt (2).
3. Remove the speedometer driven gear (1).

### Installation Procedure

1. Coat the speedometer driven gear washer with speedometer driven gear lubricant.
2. Install the speedometer driven gear (1).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the speedometer bolt and tighten to 4 N·m (36 lb in).
4. Connect the electrical connector (1) to the speedometer driven gear (2).