For 1990-2009 cars

1. Install a NEW vacuum pump gasket (3).

Note: Ensure that the vacuum pump surface and cylinder head surface are clear of old gasket material.

2. Install the vacuum pump (1).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the 4 vacuum pump bolts (2) and tighten to 11 N·m (98 lb in) .
4. Install the wiring harness bracket (1).
5. Install the 2 wiring harness bracket nuts (2) and tighten to 20 N·m (15 lb ft) .
6. Install 4 wiring harness clips (1) to the bracket (3).
7. Install the wiring harness plug (2).