For 1990-2009 cars

#### Special Tools

• | EN-6347 Bracket

• | EN-956-1 Handle / Extension

• | EN-49456 Puller

For equivalent regional tools, refer to Special Tools.

1. Install EN-6347 bracket and EN-956-1 handle (2) to fix the fuel pump drive pulley (1).
2. Remove the fuel pump drive pulley nut (3).
3. Install EN-49456 puller (2) to remove the fuel pump drive pulley (1).
4. Remove fuel pump drive pulley (4).
5. Remove the fuel injection pump drive gear key (1).