For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

1 | Rear Wheelhouse Panel Liner Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (23 lb in)
2 | Rear Wheelhouse Panel Liner Nut (Qty: 2) Tighten 2.5 N·m (23 lb in)
3 | Rear Wheelhouse Panel Liner Plastic Retainer (Qty: 2)
4 | Rear Wheelhouse Panel Liner