For 1990-2009 cars

### Removal Procedure

Warning: Refer to Brake Dust Warning in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Remove the brake drum. Refer to Brake Drum Replacement.

Caution: Do not over stretch the adjuster spring. Damage can occur if the spring is over stretched.

4. Remove the adjuster spring (1). Disengage the adjuster spring hook end from the tab on the adjuster actuator lever, then release the spring from the brake shoe web hole.
5. Release the adjuster actuator lever (1) from the adjuster assembly (2).

Remove the adjuster assembly (2).

6. Remove the adjuster assembly (2) and inspect for the following conditions:

• | Binding or seized threaded adjuster assembly.

• | Damaged or missing adjuster screw teeth.

7. Replace the adjuster assembly if any of the conditions listed are present.

### Installation Procedure

1. Install the adjuster assembly (2) to the adjuster actuator lever (1).

Turn in the adjuster as far as possible.

2. Install the adjuster spring (1). Ensure that the loop end of the spring fully engages the tab on the actuator lever.
3. Install the brake drum. Refer to Brake Drum Replacement.
4. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
5. Lower the vehicle.