For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front transmission mount through bolt (1).
3. Remove the transmission mount-to-transmission attachment bolts (1).
4. Remove the transmission mount (1) from the vehicle.

### Installation Procedure

1. Install the transmission mount (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the transmission mount bolts (1) and tighten to 62 N·m (46 lb ft).
3. Install the transmission mount through bolt (1) and tighten to 62 N·m (46 lb ft).
4. Lower the vehicle.