For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove instrument panel accessory bezel. Refer to Instrument Panel Accessory Bezel Replacement.

1 | Heater and Air Conditioning Control Screw (Qty: 2). Caution: Refer to Fastener Caution in the Preface section. Tip

• | The key should be in the OFF position when connecting the electrical connectors to ensure proper calibration.

• | Disconnect the heater and air conditioning control assembly electrical connectors.

Tighten
2.5 N·m (22 lb in)

2 | Heater and Air Conditioning Control Tip Refer to Control Module References.