For 1990-2009 cars

#### Special Tools

EN-45059 Torque Angle Sensor Kit

For equivalent regional tools, refer to Special Tools.

1. Clean the sealing surfaces.
2. Inspect for plane surface.

• | Cylinder block, cylinder head

• | Straight-edge, feeler gage

3. Install the cylinder head gasket.
4. Install the cylinder head.

Caution: Refer to Fastener Caution in the Preface section.

Note: Note the correct tightening sequence.

5. Install NEW cylinder head bolts.
6. Tighten the bolts in 5 passes. Use the EN-45059 sensor kit .

• | First pass to 25 N·m (18 lb ft)

• | Second pass to 90 degrees

• | Third pass to 90 degrees

• | Fourth pass to 90 degrees

• | Fifth pass to 45 degrees