For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Inflator Module Handling and Storage Warning in the Preface section. Warning: Following the deployment of a side impact air bag, inspect the following parts for damage. Replace these parts if necessary:

• | The seat cushion frame

• | The seat recliner, if equipped

• | The seat adjuster

• | The seat back frame

Failure to do so may cause future personal injury.

#### Preliminary Procedure

Disable the SIR system. Refer to SIR Disabling and Enabling.

1 | Front Seat Back Trim
2 | Front Seat Side Inflatable Restraint Module Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (36 lb in)
3 | Front Seat Side Inflatable Restraint Module Assembly Tip Disconnect the electrical connector.