For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove turn signal switch. Refer to Turn Signal Switch Replacement.
2. Remove windshield wiper and washer switch. Refer to Windshield Wiper and Washer Switch Replacement.
3. Remove steering wheel inflatable restraint module coil. Refer to Steering Wheel Inflatable Restraint Module Coil Replacement.

1 | Ignition Lock Cylinder Bolt Note: The ignition lock cylinder bolt tears off after reaching fixation torque.
2 | Ignition Lock Cylinder

#### Procedure

Disconnect electrical connector.