For 1990-2009 cars

#### Special Tools

• | CH-904 Base Frame

• | CH-49290 Mounting Engine/Gearbox

• | CH-49290-1 Ground Plate

• | CH-49290-4 Right Pin Bracket

• | CH-49290-5 Left Pin Bracket

• | CH-49290-6 Pin

• | CH-49290-7 Adapter Plate

• | CH-49290-8 Front Mounting Bracket Right

• | CH-49290-9 Front Mounting Bracket Left

• | CH-49290-10 Rear Mounting Bracket Right

• | CH-49290-11 Rear Mounting Bracket Left

• | CH-49290-12 Adapter Plate

• | CH-49290-14 Supporting Stand

• | CH-49290-15 Adapter Plate

• | CH-49290-16 Supporting Stand

• | CH-49290-18 Supporting Stand

For equivalent regional tools, refer to Special Tools.

### Prepare the CH-49290 for Mounting Engine

1. Install the tool components at the CH-49290-1 plate (2).

• | CH-49290-16 supporting with

| CH-49290-15 plate (3) at position 21 and V.

• | CH-49290-5 bracket (6) at position 02.

• | CH-49290-6 pin (5) at position E on the

| CH-49290-5 bracket (6).

• | CH-49290-14 supporting with

| CH-49290-12 plate (7) at position 13 and Q.

• | 2 bolts with 2 CH49290-18 supporting (10) at position 32 and position 40.

• | CH-49290-4 bracket (13) at position 01.

• | CH-49290-6 pin (14) at position B on the CH-49290-4 bracket (13).

2. Turn the CH49290-18 supporting (10), CH-49290-14 supporting (7) and CH-49290-16 supporting (3) downward.

Note: Do not Install the CH-49290-10 bracket (1), CH-49290-11 bracket (4), CH-49290-7 plate (8), CH-49290-9 bracket (9), CH-49290-7 plate (12) and CH-49290-8 bracket (11) until the tool contact the frame.

### Install Procedure

1. Raise the vehicle by its full height. Refer to Lifting and Jacking the Vehicle.
2. Remove the front compartment insulator. Refer to Front Compartment Insulator Replacement.
3. Install the CH-49290 mounting at the CH-904 frame .
4. Raise the CH-49290 mounting (1) with a jack.

Note: Ensure that the 2 CH-49290-6 pin are fixed in both holes of the sub frame.

5. Install the CH-49290-9 bracket and CH-49290-8 bracket (2) with the 2 CH-49290-7 plate (4).
6. Install the 4 bolts (3).
7. Install the CH-49290-10 bracket and CH-49290-11 bracket (5).
8. Install the 4 bolts (6).
9. Lower the jack and remove it.
10. Turn the CH-49290-14 supporting (4) upwards until it seats solidly at the front engine mount bracket (3).
11. Turn the CH-49290-16 supporting (5) upwards until it seats solidly at the rear engine mount bracket (2).
12. Turn the 2 CH49290-18 supporting (6) upwards until it seats solidly at the oil pan (1).
13. Remove the CH-904 frame from the CH-49290 mounting .

### Removal Procedure

1. Install the CH-904 frame to the CH-49290 mounting .
2. Support the CH-49290 mounting (1) with a jack.
3. Remove the 4 bolts (3).
4. Remove the CH-49290-9 bracket and CH-49290-8 bracket (2) with the 2 CH-49290-7 plate (4).
5. Remove the 4 bolts (6).
6. Remove the CH-49290-10 bracket and CH-49290-11 bracket (5).
7. Lower the CH-49290 mounting with a jack.