For 1990-2009 cars

#### Special Tools

EN-45059 Torque Angle Sensor Kit

For equivalent regional tools, refer to Special Tools.

1. Clean the 4 rear timing belt cover threads.
2. Apply threadlock to the 4 NEW rear timing belt cover bolts. Refer to Adhesives, Fluids, Lubricants, and Sealers for the recommended thread locking material.
3. Install the timing belt rear cover (1).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the 4 timing belt rear cover bolts (2) and tighten to 6 N·m (53 lb in)

Note: Two mechanics are required.

5. Install the camshaft adjuster (3) and the camshaft adjuster bolts (2) and tighten the bolts in three passes using the EN-45059 sensor kit :

Hold at the appropriate camshaft hexagon.

5.1. | First pass tighten to 65 N·m (48 lb ft)

5.2. | Second pass to 120 degrees

5.3. | Third pass to 15 degrees

6. Install the 2 camshaft adjuster closure plugs (1) and tighten to 30 N·m (22 lb ft).