For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the windshield wiper arms. Refer to Windshield Wiper Arm Replacement
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.
3. Remove the wiper drive system module.

1 | Windshield Wiper Motor Bolts (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten XX N·m (XX lb in)
2 | Windshield Wiper Motor Nut Tighten XX N·m (XX lb in)
3 | Windshield Wiper Motor Assembly