For 1990-2009 cars

#### Special Tools

EN 6625 Crankshaft Locking Device

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Open the Hood.
2. Raise the vehicle by its full height. Refer to Lifting and Jacking the Vehicle.
3. Remove the front compartment splash shield. Refer to Front Compartment Splash Shield Replacement.
4. Remove the drive belt. Refer to Drive Belt Replacement.
5. Remove the bolt (1).
6. Install the EN 6625 locking device (2) to lock the crankshaft.
7. Install the bolt (1).
8. Remove the crankshaft balancer bolt (1).
9. Remove the crankshaft balancer (2).

### Installation Procedure

1. Install the crankshaft balancer (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the NEW crankshaft balancer bolt (1) and tighten to 95 N·m (70 lb ft) + 45 degrees + 15 degrees.
3. Remove the bolt (1).
4. Remove EN 6625 locking device (2) to unlock the crankshaft.
5. Install the bolt (1) and tighten to 75 N·m (56 lb ft).
6. Install the drive belt. Refer to Drive Belt Replacement.
7. Install the front compartment splash shield. Refer to Front Compartment Splash Shield Replacement.
8. Lower the vehicle by its full height. Refer to Lifting and Jacking the Vehicle.
9. Close the hood.