For 1990-2009 cars

## Fastener Tightening Specifications 2.0L Diesel LLW

Application | Specification
--- | ---
Metric | English
Charge Air Cooler Inlet Hose Bolt | 10 N·m | 89 lb in
Charge Air Cooler Inlet Hose Clamp Bolt | 10 N·m | 89 lb in
Charge Air Cooler Outlet Hose Clamp | 7 N·m | 62 lb in
Coolant Return Pipe Retaining Bolt | 9 N·m | 80 lb in
Coolant Temperature Sensor | 35 N·m | 26 lb in
Engine Coolant Air Bleed Hose Bolt | 9 N·m | 80 lb in
Engine Coolant Fan Motor Bolt | 4 N·m | 36 lb in
Engine Oil Cooler Hose Heat Shield Nut | 33 N·m | 25 lb ft
Engine Thermostat Housing Bolt Qty 2 | 23 N·m | 17 lb ft
Engine Thermostat Housing Bolt Qty 1 | 8 N·m | 71 lb in
Exhaust Gas Recirculation Cooling Pipe Bolt | 20 N·m | 15 lb ft
Exhaust Gas Recirculation Cooling Pipe Nut | 33 N·m | 25 lb ft
Radiator Support Bracket Bolt | 22 N·m | 17 lb ft
Water Pump Housing Bolt | 11 N·m | 97 lb in

## Fastener Tightening Specifications 1.6L LXV

Application | Specification
--- | ---
Metric | English
Engine Coolant Fan Motor Bolt | 3 N·m | 26 lb in
Engine Coolant Fan Resistor Bolt | 4 N·m | 36 lb in
Engine Oil Cooler Pipe Bolt | 8 N·m | 71 lb in
Engine Oil Cooler Housing Bolt | 25 N·m | 19 lb ft
Engine Coolant Thermostat Bolt | 8 N·m | 71 lb in
Engine Coolant Thermostat Bypass Pipe Bolt | 8 N·m | 71 lb in
Engine Coolant Thermostat Housing Bolt | 8 N·m | 71 lb in
Hood Hold Open Rod Retainer Bracket Bolt | 22 N·m | 17 lb ft
Radiator Bolt | 22 N·m | 17 lb ft
Radiator Bracket Bolt | 25 N·m | 18 lb ft
Radiator Hose Clamp | 3.5 N·m | 31 lb in
Water Pump Housing Bolt | 8 N·m | 71 lb in
Water Pump Pulley Bolt | 20 N·m | 15 lb ft