For 1990-2009 cars

Note: Lubricate the NEW camshaft position actuator solenoid valve seals with NEW engine oil. Refer to Adhesives, Fluids, Lubricants, and Sealers.

1. Install NEW camshaft position actuator solenoid valve seals (3).
2. Install the camshaft position actuator solenoid valves (2).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the camshaft position actuator solenoid valve bolts (1) and tighten to 6 N·m (52 lb in).