For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Side Door Inside Handle Bolt Finish Cap

#### Procedure

Pull handle back to remove cap. Use suitable tool to unsnap.

2 | Rear Side Door Inside Handle Screw Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m(X lb in)
3 | Rear Side Door Trim Clip (Qty: 6) Tighten X N·m(X lb in)
4 | Rear Side Door Trim Assembly

#### Procedure

1. Pull upwards on the door lock retainer cable to disengage.
2. Disconnect the electrical connectors.