For 1990-2009 cars

### Removal Procedure

Warning: Refer to SIR Warning in the Preface section.

Warning: Replace the passenger presence system as a complete assembly to prevent possible injury to the occupant. The bladder, the pressure sensor, the seat cushion, and the control module are assembled and calibrated as a unit. Using only some of the components in the service kit will cause the passenger presence system to operate improperly.

1. Remove front seat adjuster, if equipped. Refer to Front Seat Adjuster Replacement.
2. Remove driver or passenger seat. Refer to Driver or Passenger Seat Replacement.
3. Remove seat cushion inner trim panel. Refer to Front Seat Cushion Inner Trim Panel Replacement.
4. Remove seat cushion outer trim panel. Refer to Front Seat Cushion Outer Trim Panel Replacement.
5. Detach cushion cover from backrest below.
6. Release and disconnect wiring harness plug (1), if equipped.
7. Remove front seat backrest screw (2) (Qty: 4).
8. Remove backrest.
9. Detach cushion cover from seat frame all the way round.
10. Remove cushion cover with pad from frame.
11. Remove cushion cover from pad.

### Installation Procedure

1. Install cushion cover to pad.
2. Install cushion cover with pad to frame.
3. Attach cushion cover from seat frame all the way round.
4. Install backrest.

Caution: Refer to Fastener Caution in the Preface section.

5. Tighten screw (2) (Qty: 4).

Tighten
XX N·m (XX lb in).

6. Connect and latch wiring harness plug (1), if equipped.
7. Attach cushion cover to backrest below.

1. Install seat cushion outer trim panel. Refer to Front Seat Cushion Outer Trim Panel Replacement.
2. Install seat cushion inner trim panel. Refer to Front Seat Cushion Inner Trim Panel Replacement.
3. Install driver or passenger seat. Refer to Driver or Passenger Seat Replacement.
4. Install front seat adjuster, if equipped. Refer to Front Seat Adjuster Replacement.