For 1990-2009 cars

Checks | Causes
--- | ---
Case Assembly (50) |

• | Inspect for cracked or broken Case (50)

• | Inspect for stripped or sheared splines

• | Inspect for missing Lube Orifice Plug

• | Inspect for binding Manual Shift Detent Lever Assembly (609)

• | Inspect for missing Manual Shift Shaft Pin (611)

• | Inspect for missing Manual Shaft Lever Pin (610)

• | Inspect for interference or binding Park Pawl Actuator Assembly (607)

• | Inspect for broken or disengaged 1-2-3-4 Clutch Backing Plate Retainer Ring (561)

• | Inspect for loose or damaged case bushing

Drive Link Lubrication Scoop (55) | Inspect for leaking, damaged or missing Drive Link Lube Scoop Seals (59)
Torque Converter (28) |

• | Inspect for stripped or sheared splines on Turbine Shaft

• | Inspect for missing Torque Converter to Flywheel bolts

• | Inspect for damaged or disengaged Torque Converter Hub to Oil Pump Drive Gear

Torque Converter Housing (208) |

• | Inspect for stripped or sheared Differential Ring Gear splines

• | Inspect for broken or disengaged Differential Ring Gear Retainer (206)

• | Inspect for loose, missing or broken Torque Converter and Differential Housing bolts (26)

• | Inspect for loose, missing or broken Fluid Pump bolts (200)

35R/456 Housing Assembly (516) |

• | Inspect for damaged or broken Input Shaft Thrust Bearing Assembly (538)

• | Inspect for stripped or sheared splines on the Input Shaft to the 3-5 Reverse/4-5-6 Clutch Housing (516)

Oil Pump Assembly (201) |

• | Inspect for fluid leaks / improper fluid level

• | Inspect for leaking Fluid Outlet Seal Assembly (24)

• | Inspect for loose or missing Oil Pump Bolts (200)

• | Inspect for damaged, restricted or improperly installed Oil Filter Assembly (203)

• | Inspect for damaged or leaking Oil Filter Neck Seal

Low & Reverse Clutch Assembly (543) | Inspect for stripped or sheared splines to the Reaction Carrier (567)
Input Carrier Assembly (570) |

• | Inspect for stripped or sheared castle splines to ring gear

• | Inspect for improperly installed carrier pinion gear pins

• | Inspect for damaged or broken Pinion Gears

• | Inspect for stripped or sheared splines on the Input Sun Gear (571)

• | Inspect for damaged or broken Output Internal Gear

• | Inspect for broken or disengaged Output Internal Gear Retainer Ring

• | Inspect for damaged or broken Input Carrier Thrust Bearing Assembly (568) and Output Carrier Thrust Bearing Assembly (573)

• | Inspect for damaged or broken Input Carrier Thrust Bearings (569, 572)

Reaction Carrier Assembly (567) |

• | Inspect for stripped or sheared Reaction Carrier Assembly (567) splines

• | Inspect for damaged or broken Input Carrier Thrust Bearings (568)

• | Inspect for damaged or broken Pinion Gear teeth

• | Inspect for damaged or broken Reaction Internal Gear teeth

• | Inpsect for disengaged or broken Reaction Internal Gear retainer ring

Reaction Sun Gear Assembly (566) |

• | Inspect for damaged or broken weld at Sun Gear

• | Inspect for loose or worn Reaction Sun Gear Assembly bushing

Output Carrier Assembly (574) |

• | Inspect for stripped or sheared splines to reaction internal ring gear

• | Inspect for damaged or broken Input Sun Gear Thrust Bearings (572)

• | Inspect for damaged or broken Pinion Gear teeth

• | Inspect for damaged or broken Input Carrier Thrust Bearings (573)

• | Inspect for broken or damaged Output Internal Gear

Output Sun Gear Assembly (555) |

• | Inspect for stripped or sheared Output Sun Gear Assembly (555) splines

• | Inspect for broken Output Sun Gear Assembly (555) hub or weld

Low-Reverse and 1-2-3-4 Clutch Housing (551) | Inspect for disengaged or broken 1-2-3-4 Clutch Piston Spring Retainer (554)
Drive Link Assembly (225) |

• | Inspect for broken, worn or damaged Drive Link Assembly (225)

• | Inspect for broken, worn or damaged Drive Sprocket (224)

• | Inspect for broken, worn or damaged Driven Sprocket Assembly (229)

• | Inspect for broken Drive Gear Hub (222)

Differential Carrier Assembly (232) |

• | Inspect for stripped or sheared splines on Differential Side Gear

• | Inspect for stripped or sheared splines Final Drive Sun Gear (230)

• | Inspect for stripped or sheared splines Differential Carrier to PTU (AWD only)

• | Inspect for stripped broken or disengaged Final Drive Retainer (581)

• | Inspect for damaged or broken Pinion Gear teeth

• | Inpsect for damaged or broken Final Drive Rollers (585)

• | Inspect for broken, worn or damaged Final Drive Inner and Outer Thrust Washers (584)