For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disable the SIR system. Refer to SIR Disabling and Enabling.

1 | Windshield Garnish Molding Assembly

#### Procedure

1. Tabs must be installed prior to retainers.
2. Tabs to be fully seated in I/P trim panel retainer and valance panel.
3. Disconnect electrical connectors.
4. Ensure the tether is reattached when installed.