For 1990-2009 cars

### Removal Procedure

1. Remove the drive belt. Refer to Generator and Air Conditioning Compressor and Power Steering Pump Belt Replacement .
2. Lower the vehicle at full height. Refer to Lifting and Jacking the Vehicle .
3. Remove the drive belt idler pulley bolt (2).
4. Remove drive belt idler pulley (1).

### Installation Procedure

1. Install the drive belt idler pulley (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the drive belt idler pulley bolt and tighten to 52 N·m (38 lb ft) .
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
4. Install the drive belt. Refer to Generator and Air Conditioning Compressor and Power Steering Pump Belt Replacement .