For 1990-2009 cars

### Removal Procedure

Warning: Refer to Brake Fluid Irritant Warning in the Preface section.

Caution: Refer to Brake Fluid Effects on Paint and Electrical Components Caution in the Preface section.

Warning: Do not place fingers in front of the caliper piston(s) in an attempt to catch or protect it when applying compressed air. The piston(s) can fly out with force and could result in serious bodily injury.

Caution: Use clean cloths to pad interior of caliper housing during piston removal. Use just enough air to ease the pistons out of the bores. If the pistons are blown out, even with the padding provided, it may be damaged.

1. Inspect the fluid level in the brake master cylinder reservoir.
2. If the brake fluid level is midway between the maximum-full point and the minimum allowable level, no brake fluid needs to be removed from the reservoir before proceeding.
3. If the brake fluid level is higher than midway between the maximum-full point and the minimum allowable level, remove brake fluid to the midway point before proceeding.
4. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
5. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
6. Remove the brake hose to caliper bolt (2) from the brake caliper.
7. Remove the brake hose (1) from the brake caliper.
8. Remove and discard the 2 copper brake hose gaskets (3). These gaskets may be stuck to the brake caliper and/or the brake hose end.
9. Cap or plug the opening in the brake caliper and the brake hose to prevent fluid loss and contamination.
10. Remove the 2 brake caliper pin bolts (1).
11. Remove the park brake cable (1) from the caliper (2).
12. Remove the brake caliper (2) from the brake caliper bracket.

### Installation Procedure

1. Inspect the caliper slide boots for cuts, tears, or deterioration. If damaged, replace the slides and boots. Refer to Rear Disc Brake Hardware Replacement.
2. Install the brake caliper to the brake caliper bracket.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the 2 brake caliper pin bolts (1) and tighten to XX N·m (XX lb in).
4. Install the park brake cable (1) to the caliper (2).
5. Remove the caps or plugs from the brake caliper opening and the brake hose.

Note: DO NOT reuse the copper brake hose gaskets.

6. Install NEW copper brake hose gaskets (3) to the brake hose-to-caliper bolt (2) and to the brake hose.
7. Install the brake hose and the brake hose-to-caliper bolt to the brake caliper and tighten the bolt to XX N·m (XX lb in).
8. Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding.
9. With the engine OFF, gradually apply the brake pedal to approximately 2/3 of its travel distance.
10. Slowly release the brake pedal.
11. Wait 15 seconds, then repeat steps 9 and 10 until a firm brake pedal is obtained. This will properly seat the brake caliper pistons and brake pads.
12. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
13. Lower the vehicle.
14. Apply and release the park brake lever 4 times.