For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the control solenoid valve and transmission control module assembly. Refer to Control Solenoid Valve and Transmission Control Module Assembly Replacement.

1 | Fluid Level Control Valve
2 | Fluid Level Control Valve Gasket
3 | Control Valve Body Bolt M6 x 60 (Qty: 9) Caution: Refer to Fastener Caution in the Preface section. Tip Tighten in specified sequence. Tighten
12 N·m (107 lb in)

4 | Control Valve Body Bolt M6 x 53 (Qty: 2) Tip Tighten in specified sequence. Tighten 12 N·m (107 lb in)
5 | Control Valve Body Assembly
6 | Control Valve Body Spacer Plate Assembly
7 | Manual Shaft Detent Spring Bolt M6 x 16 (Qty: 1) Tighten 12 N·m (107 lb in)
8 | Manual Shaft Detent Lever Spring Assembly
9 | 1-2-3-4 Clutch Fluid Passage Seal Tip Discard the seal. It is not reusable.
10 | Low/Reverse Clutch Fluid Passage Seal Tip Discard the seal. It is not reusable.