For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove engine cover. Refer to Engine Cover Replacement.
2. Remove air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
4. Install mounting engine / transmission. Refer to Engine/Transmission Mounting

1 | Engine Mount Bracket Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Engine Mount
3 | Engine Mount Bolt (Qty: 2) Tighten 62 N·m (46 lb ft)
4 | Engine Mount Nut Tighten 58 N·m (43 lb ft)