For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove front bumper fascia guide. Refer to Front Bumper Fascia Replacement.
3. Remove the wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
4. Remove the headlamp. Refer to Headlamp Replacement.
5. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.

1 | Front Fender Bolt (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (70 lb in)
2 | Front Fender Bolt

#### Procedure

Open the door to access bolt.

Tighten
8 N·m (70 lb in)

3 | Front Fender Bold (Qty 2) Tip Simply loosen the bolt rather than remove. Tighten 8 N·m(70 lb in)
4 | Front Fender