For 1990-2009 cars

## Exhaust Gas Recirculation Cooling Pipe Replacement - Lower 2.0L Diesel LLW

Callout | Component Name
--- | ---
1 | Exhaust Gas Recirculation Cooling Pipe Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
2 | Exhaust Gas Recirculation Cooling Pipe Nut (Qty: 2) Tighten 20 N·m (15 lb ft)
3 | Exhaust Gas Recirculation Cooling Pipe Gaskets
4 | Exhaust Gas Recirculation Cooling Pipe - Lower