For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptors

DTC P2226 03: Barometric Pressure (BARO) Sensor Circuit Voltage Below Threshold
DTC P2226 07: Barometric Pressure (BARO) Sensor Circuit Voltage Above Threshold

### Circuit/System Description

The BARO sensor is integrated within the engine control module (ECM). The barometric pressure (BARO) sensor responds to changes in altitude and atmospheric conditions. The BARO sensor provides the ECM an indication of barometric pressure. The BARO sensor provides a voltage signal to the ECM relative to the atmospheric pressure changes. The ECM monitors the BARO sensor signal for a voltage outside of the normal range.

### Conditions for Running the DTC

The ignition is ON or the engine is running.

### Conditions for Setting the DTC

#### P2226 03

• | The ECM detects that the BARO sensor voltage is less than 2.1 volts.

• | The condition exists for greater than 0.5 seconds.

#### P2226 07

• | The ECM detects that the BARO sensor voltage is greater than 4.7 volts.

• | The condition exists for greater than 0.5 seconds.

### Action Taken When the DTC Sets

DTCs P2226 is a Type B DTC.

### Conditions for Clearing the MIL/DTC

DTCs P2226 is a Type B DTC.

### Reference Information

#### Schematic Reference

Engine Controls Schematics

#### Connector End View Reference

Component Connector End Views

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

#### Scan Tool Reference

Control Module References

### Circuit/System Verification

Note: If you were sent here from P0069, proceed to Circuit System Testing.

1. Engine running, observe the DTC information with a scan tool. DTCs P2226 should not set.
2. Operate the vehicle within the Conditions for Running the DTC to verify the DTC does not reset. You may also operate the vehicle within the conditions that you observed from the Freeze Frame/Failure Records data.

### Circuit/System Testing

1. Inspect the atmospheric vent on the ECM case for one of the following conditions:

• | Moisture in the vent inlet

• | Debris in the vent inlet

⇒ | If a condition exists, attempt to clean or dry the atmospheric inlet.

2. Engine running, observe the DTC information with a scan tool. DTCs P0069 or P2226 should not set.

⇒ | If DTC P0069 or P2226 sets, replace the K20 ECM.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

Control Module References for engine control module replacement, setup, and programming