For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the intake air duct bolt (2).
3. Remove the intake air duct (1)

### Installation Procedure

1. Install the intake air duct (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the intake air duct bolt (2) and tighten the to 5 N·m(45 lb in)
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement.