For 1990-2009 cars

#### Special Tools

EN 49424 Remover and Installer Ignition Module

For equivalent regional tools, refer to Special Tools.

Note: When installing a new DIS ignition module it is not necessary to replace the gaskets.

1. Install the EN 49424 remover / installer .
2. Install the ignition coil (1) and the NEW gaskets (2).

Caution: Refer to Fastener Caution in the Preface section.

Note: Note the arrow on the cover.

3. Install the 2 ignition coil bolts an tighten to 8 N·m (71 lb in).
4. Install the cover of the ignition coil in the direction of the arrow.